<?xml version="1.0" ?>
<node xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xs="http://www.w3.org/2001/XMLSchema" xmlns:altera="http://www.altera.com/XMLSchema/Qsys/SystemTree">
  <instanceKey xsi:type="xs:string">pll</instanceKey>
  <instanceData xsi:type="data">
    <parameters></parameters>
    <interconnectAssignments></interconnectAssignments>
    <className>pll</className>
    <version>1.0</version>
    <name>pll</name>
    <uniqueName>pll</uniqueName>
    <nonce>0</nonce>
    <incidentConnections></incidentConnections>
  </instanceData>
  <children>
    <node>
      <instanceKey xsi:type="xs:string">iopll_0</instanceKey>
      <instanceData xsi:type="data">
        <parameters>
          <parameter>
            <name>bandwidth_mode</name>
            <value>BANDWIDTH_MODE_AUTO</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en0</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en1</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en10</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en11</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en12</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en13</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en14</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en15</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en16</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en17</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en2</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en3</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en4</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en5</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en6</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en7</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en8</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_bypass_en9</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div0</name>
            <value>64</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div1</name>
            <value>255</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div10</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div11</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div12</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div13</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div14</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div15</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div16</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div17</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div2</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div3</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div4</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div5</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div6</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div7</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div8</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_hi_div9</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src0</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src1</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src10</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src11</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src12</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src13</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src14</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src15</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src16</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src17</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src2</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src3</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src4</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src5</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src6</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src7</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src8</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_in_src9</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div0</name>
            <value>64</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div1</name>
            <value>255</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div10</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div11</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div12</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div13</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div14</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div15</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div16</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div17</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div2</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div3</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div4</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div5</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div6</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div7</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div8</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_lo_div9</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en0</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en1</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en10</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en11</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en12</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en13</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en14</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en15</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en16</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en17</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en2</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en3</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en4</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en5</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en6</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en7</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en8</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_odd_div_duty_en9</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst0</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst1</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst10</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst11</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst12</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst13</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst14</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst15</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst16</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst17</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst2</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst3</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst4</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst5</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst6</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst7</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst8</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_ph_mux_prst9</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst0</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst1</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst10</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst11</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst12</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst13</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst14</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst15</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst16</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst17</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst2</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst3</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst4</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst5</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst6</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst7</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst8</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>c_cnt_prst9</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>cal_code_hex_file</name>
            <value>iossm.hex</value>
          </parameter>
          <parameter>
            <name>cal_converge</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>cal_error</name>
            <value>cal_clean</value>
          </parameter>
          <parameter>
            <name>cascade_mode</name>
            <value>CASCADE_MODE_STANDALONE</value>
          </parameter>
          <parameter>
            <name>clock_name_0</name>
            <value>outclk0</value>
          </parameter>
          <parameter>
            <name>clock_name_1</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_2</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_3</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_4</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_5</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_6</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_7</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_8</name>
            <value></value>
          </parameter>
          <parameter>
            <name>clock_name_global</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_0</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_1</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_2</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_3</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_4</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_5</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_6</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_7</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_name_global_8</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>clock_to_compensate</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>compensation_clk_source</name>
            <value>COMPENSATION_CLK_SOURCE_UNUSED</value>
          </parameter>
          <parameter>
            <name>compensation_mode</name>
            <value>COMPENSATION_MODE_DIRECT</value>
          </parameter>
          <parameter>
            <name>divide_factor0</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor1</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor2</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor3</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor4</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor5</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor6</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor7</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>divide_factor8</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>dprio_interface_sel</name>
            <value>3</value>
          </parameter>
          <parameter>
            <name>duty_cycle0</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle1</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle10</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle11</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle12</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle13</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle14</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle15</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle16</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle17</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle2</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle3</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle4</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle5</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle6</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle7</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle8</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>duty_cycle9</name>
            <value>50</value>
          </parameter>
          <parameter>
            <name>eff_m_cnt</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>fb_clk_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>fb_clk_fractional_div_den</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>fb_clk_fractional_div_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>fb_clk_fractional_div_value</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>fb_clk_m_div</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>fractional_vco_multiplier</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_active_clk</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle0</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle1</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle10</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle11</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle12</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle13</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle14</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle15</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle16</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle17</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle2</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle3</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle4</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle5</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle6</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle7</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle8</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle9</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range0</name>
            <value>49.33,49.44,49.54,50.0,50.39,50.5</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range1</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range10</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range11</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range12</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range13</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range14</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range15</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range16</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range17</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range2</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range3</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range4</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range5</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range6</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range7</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range8</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_duty_cycle_range9</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency0</name>
            <value>25.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency1</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency10</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency11</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency12</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency13</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency14</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency15</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency16</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency17</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency2</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency3</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency4</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency5</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency6</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency7</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency8</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency9</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range0</name>
            <value>24.95935,24.96,24.96063,25.0,25.03937,25.04</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range1</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range10</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range11</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range12</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range13</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range14</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range15</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range16</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range17</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range2</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range3</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range4</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range5</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range6</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range7</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range8</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_output_clock_frequency_range9</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift0</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg0</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range0</name>
            <value>0.0,0.4,0.4,0.4,0.4,0.4</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_deg_range9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range0</name>
            <value>0.0,39.1,39.7,40.3,41.0,41.7</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_actual_phase_shift_range9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src0</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src1</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src2</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src3</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src4</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src5</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src6</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src7</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_c_cnt_in_src8</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_cal_code_hex_file</name>
            <value>iossm.hex</value>
          </parameter>
          <parameter>
            <name>gui_cal_converge</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cal_error</name>
            <value>cal_clean</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter0</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter1</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter10</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter11</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter12</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter13</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter14</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter15</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter16</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter17</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter2</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter3</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter4</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter5</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter6</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter7</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter8</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_counter9</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_cascade_outclk_index</name>
            <value>5</value>
          </parameter>
          <parameter>
            <name>gui_clk_bad</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_global</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_instantiation</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string0</name>
            <value>outclk0</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string1</name>
            <value>outclk1</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string10</name>
            <value>outclk10</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string11</name>
            <value>outclk11</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string12</name>
            <value>outclk12</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string13</name>
            <value>outclk13</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string14</name>
            <value>outclk14</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string15</name>
            <value>outclk15</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string16</name>
            <value>outclk16</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string17</name>
            <value>outclk17</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string2</name>
            <value>outclk2</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string3</name>
            <value>outclk3</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string4</name>
            <value>outclk4</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string5</name>
            <value>outclk5</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string6</name>
            <value>outclk6</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string7</name>
            <value>outclk7</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string8</name>
            <value>outclk8</value>
          </parameter>
          <parameter>
            <name>gui_clock_name_string9</name>
            <value>outclk9</value>
          </parameter>
          <parameter>
            <name>gui_clock_to_compensate</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>gui_debug_mode</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_device_component</name>
            <value>A5EB013BB23BE4SCS</value>
          </parameter>
          <parameter>
            <name>gui_device_family</name>
            <value>Agilex 5</value>
          </parameter>
          <parameter>
            <name>gui_device_iobank_rev</name>
            <value>IO96B_REVB1</value>
          </parameter>
          <parameter>
            <name>gui_device_speed_grade</name>
            <value>4</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c0</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c1</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c10</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c11</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c12</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c13</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c14</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c15</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c16</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c17</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c2</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c3</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c4</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c5</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c6</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c7</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c8</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_c9</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_divide_factor_n</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_dps_cntr</name>
            <value>C0</value>
          </parameter>
          <parameter>
            <name>gui_dps_dir</name>
            <value>Positive</value>
          </parameter>
          <parameter>
            <name>gui_dps_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_dsm_out_sel</name>
            <value>1st_order</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle0</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle1</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle10</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle11</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle12</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle13</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle14</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle15</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle16</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle17</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle2</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle3</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle4</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle5</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle6</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle7</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle8</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_duty_cycle9</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_en_adv_params</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_dps_ports</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_extclkout_ports</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_hvio_reconf</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_iossm_reconf</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_lvds_ports</name>
            <value>Disabled</value>
          </parameter>
          <parameter>
            <name>gui_en_periphery_ports</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_phout_ports</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_en_reconf</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_cascade_in</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_cascade_out</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_mif_dps</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_output_counter_cascading</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_permit_cal</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_enable_upstream_out_clk</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_existing_mif_file_path</name>
            <value>~/pll.mif</value>
          </parameter>
          <parameter>
            <name>gui_extclkout_0_source</name>
            <value>C0</value>
          </parameter>
          <parameter>
            <name>gui_extclkout_1_source</name>
            <value>C0</value>
          </parameter>
          <parameter>
            <name>gui_extclkout_source</name>
            <value>C0</value>
          </parameter>
          <parameter>
            <name>gui_feedback_clock</name>
            <value>Global Clock</value>
          </parameter>
          <parameter>
            <name>gui_fix_vco_frequency</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_fixed_vco_frequency</name>
            <value>600.0</value>
          </parameter>
          <parameter>
            <name>gui_fixed_vco_frequency_ps</name>
            <value>1667.0</value>
          </parameter>
          <parameter>
            <name>gui_frac_multiply_factor</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_fractional_cout</name>
            <value>32</value>
          </parameter>
          <parameter>
            <name>gui_include_iossm</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_location_type</name>
            <value>I/O Bank</value>
          </parameter>
          <parameter>
            <name>gui_lock_setting</name>
            <value>Low Lock Time</value>
          </parameter>
          <parameter>
            <name>gui_mif_config_name</name>
            <value>unnamed</value>
          </parameter>
          <parameter>
            <name>gui_mif_gen_options</name>
            <value>Generate New MIF File</value>
          </parameter>
          <parameter>
            <name>gui_multiply_factor</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>gui_multiply_fraction</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>gui_new_mif_file_path</name>
            <value>~/pll.mif</value>
          </parameter>
          <parameter>
            <name>gui_number_of_clocks</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_operation_mode</name>
            <value>direct</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency0</name>
            <value>25.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency1</name>
            <value>12.288</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency10</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency11</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency12</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency13</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency14</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency15</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency16</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency17</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency2</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency3</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency4</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency5</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency6</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency7</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency8</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency9</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps0</name>
            <value>20000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps1</name>
            <value>81380.208</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps10</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps11</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps12</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps13</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps14</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps15</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps16</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps17</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps2</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps3</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps4</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps5</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps6</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps7</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps8</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_output_clock_frequency_ps9</name>
            <value>10000.0</value>
          </parameter>
          <parameter>
            <name>gui_parameter_table_hex_file</name>
            <value>seq_params_sim.hex</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift0</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg0</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phase_shift_deg9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>gui_phout_division</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_pll_auto_reset</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_pll_bandwidth_preset</name>
            <value>Low</value>
          </parameter>
          <parameter>
            <name>gui_pll_cal_done</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_pll_cascading_mode</name>
            <value>adjpllin</value>
          </parameter>
          <parameter>
            <name>gui_pll_freqcal_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>gui_pll_freqcal_req_flag</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>gui_pll_m_cnt_in_src</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>gui_pll_mode</name>
            <value>Integer-N PLL</value>
          </parameter>
          <parameter>
            <name>gui_pll_tclk_mux_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_pll_tclk_sel</name>
            <value>pll_tclk_m_src</value>
          </parameter>
          <parameter>
            <name>gui_pll_type</name>
            <value>S10_Physical</value>
          </parameter>
          <parameter>
            <name>gui_pll_vco_freq_band_0</name>
            <value>pll_freq_clk0_band18</value>
          </parameter>
          <parameter>
            <name>gui_pll_vco_freq_band_1</name>
            <value>pll_freq_clk1_band18</value>
          </parameter>
          <parameter>
            <name>gui_prot_mode</name>
            <value>UNUSED</value>
          </parameter>
          <parameter>
            <name>gui_ps_units0</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units1</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units10</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units11</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units12</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units13</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units14</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units15</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units16</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units17</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units2</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units3</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units4</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units5</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units6</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units7</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units8</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_ps_units9</name>
            <value>ps</value>
          </parameter>
          <parameter>
            <name>gui_refclk1_frequency</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>gui_refclk_might_change</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_refclk_switch</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_reference_clock_frequency</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>gui_reference_clock_frequency_ps</name>
            <value>20000.0</value>
          </parameter>
          <parameter>
            <name>gui_set_locked_as_reset</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_simulation_type</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>gui_skip_sdc_generation</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_switchover_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>gui_switchover_mode</name>
            <value>Automatic Switchover</value>
          </parameter>
          <parameter>
            <name>gui_use_NDFB_modes</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_use_coreclk</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_use_fractional_division</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_use_locked</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>gui_use_logical</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_use_slvs_refclk</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_use_slvs_refclk1</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>gui_user_base_address</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>gui_usr_device_speed_grade</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>gui_vco_frequency</name>
            <value>600.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp0</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp1</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp10</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp11</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp12</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp13</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp14</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp15</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp16</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp17</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp2</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp3</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp4</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp5</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp6</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp7</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp8</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_duty_cycle_fp9</name>
            <value>50.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp0</name>
            <value>25.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp1</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp10</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp11</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp12</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp13</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp14</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp15</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp16</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp17</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp2</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp3</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp4</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp5</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp6</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp7</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp8</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_output_clock_frequency_fp9</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp0</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp1</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp10</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp11</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp12</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp13</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp14</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp15</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp16</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp17</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp2</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp3</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp4</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp5</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp6</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp7</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp8</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_phase_shift_fp9</name>
            <value>0.0</value>
          </parameter>
          <parameter>
            <name>hp_actual_vco_frequency_fp</name>
            <value>600.0</value>
          </parameter>
          <parameter>
            <name>hp_number_of_family_allowable_clocks</name>
            <value>9</value>
          </parameter>
          <parameter>
            <name>hp_parameter_update_message</name>
            <value></value>
          </parameter>
          <parameter>
            <name>hp_previous_num_clocks</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>hp_qsys_scripting_mode</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>include_iossm</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>iossm_nios_sim_clk_period_ps</name>
            <value>1333</value>
          </parameter>
          <parameter>
            <name>lock_mode</name>
            <value>low_lock_time</value>
          </parameter>
          <parameter>
            <name>m_cnt_bypass_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>m_cnt_hi_div</name>
            <value>32</value>
          </parameter>
          <parameter>
            <name>m_cnt_lo_div</name>
            <value>32</value>
          </parameter>
          <parameter>
            <name>m_cnt_odd_div_duty_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>merging_permitted</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>mifTable_names</name>
            <value>The MIF file specified does not yet exist</value>
          </parameter>
          <parameter>
            <name>mifTable_values</name>
            <value></value>
          </parameter>
          <parameter>
            <name>mimic_fbclk_type</name>
            <value>gclk</value>
          </parameter>
          <parameter>
            <name>multiply_factor</name>
            <value>64</value>
          </parameter>
          <parameter>
            <name>n_cnt_bypass_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>n_cnt_hi_div</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>n_cnt_lo_div</name>
            <value>256</value>
          </parameter>
          <parameter>
            <name>n_cnt_odd_div_duty_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>number_of_clocks</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>number_of_outclks</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>operation_mode</name>
            <value>direct</value>
          </parameter>
          <parameter>
            <name>out_clk_0_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_0_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_0_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_0_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_0_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_0_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_0_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_0_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_1_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_1_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_1_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_1_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_1_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_1_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_1_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_1_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_2_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_2_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_2_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_2_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_2_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_2_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_2_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_2_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_3_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_3_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_3_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_3_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_3_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_3_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_3_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_3_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_4_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_4_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_4_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_4_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_4_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_4_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_4_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_4_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_5_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_5_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_5_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_5_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_5_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_5_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_5_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_5_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_6_c_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_6_core_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_6_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_6_dutycycle_den</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>out_clk_6_dutycycle_num</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>out_clk_6_freq</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_6_phase_ps</name>
            <value>1000000000</value>
          </parameter>
          <parameter>
            <name>out_clk_6_phase_shifts</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_cascading_source</name>
            <value>OUT_CLK_CASCADING_SOURCE_UNUSED</value>
          </parameter>
          <parameter>
            <name>out_clk_external_0_source</name>
            <value>OUT_CLK_EXTERNAL_0_SOURCE_UNUSED</value>
          </parameter>
          <parameter>
            <name>out_clk_external_1_source</name>
            <value>OUT_CLK_EXTERNAL_1_SOURCE_UNUSED</value>
          </parameter>
          <parameter>
            <name>out_clk_periph_0_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_periph_0_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>out_clk_periph_1_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>out_clk_periph_1_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency0</name>
            <value>25.0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency1</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency10</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency11</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency12</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency13</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency14</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency15</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency16</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency17</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency2</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency3</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency4</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency5</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency6</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency7</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency8</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>output_clock_frequency9</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>parameterTable_names</name>
            <value>M-Counter Divide Setting,N-Counter Divide Setting,VCO Frequency,C-Counter-0 Divide Setting,C-Counter-1 Divide Setting,C-Counter-2 Divide Setting,C-Counter-3 Divide Setting,C-Counter-4 Divide Setting,C-Counter-5 Divide Setting,C-Counter-6 Divide Setting,C-Counter-7 Divide Setting,C-Counter-8 Divide Setting,PLL Auto Reset,M-Counter Hi Divide,M-Counter Lo Divide,M-Counter Even Duty Enable,M-Counter Bypass Enable,N-Counter Hi Divide,N-Counter Lo Divide,N-Counter Even Duty Enable,N-Counter Bypass Enable,C-Counter-0 Hi Divide,C-Counter-1 Hi Divide,C-Counter-2 Hi Divide,C-Counter-3 Hi Divide,C-Counter-4 Hi Divide,C-Counter-5 Hi Divide,C-Counter-6 Hi Divide,C-Counter-7 Hi Divide,C-Counter-8 Hi Divide,C-Counter-0 Lo Divide,C-Counter-1 Lo Divide,C-Counter-2 Lo Divide,C-Counter-3 Lo Divide,C-Counter-4 Lo Divide,C-Counter-5 Lo Divide,C-Counter-6 Lo Divide,C-Counter-7 Lo Divide,C-Counter-8 Lo Divide,C-Counter-0 Even Duty Enable,C-Counter-1 Even Duty Enable,C-Counter-2 Even Duty Enable,C-Counter-3 Even Duty Enable,C-Counter-4 Even Duty Enable,C-Counter-5 Even Duty Enable,C-Counter-6 Even Duty Enable,C-Counter-7 Even Duty Enable,C-Counter-8 Even Duty Enable,C-Counter-0 Bypass Enable,C-Counter-1 Bypass Enable,C-Counter-2 Bypass Enable,C-Counter-3 Bypass Enable,C-Counter-4 Bypass Enable,C-Counter-5 Bypass Enable,C-Counter-6 Bypass Enable,C-Counter-7 Bypass Enable,C-Counter-8 Bypass Enable,C-Counter-0 Preset,C-Counter-1 Preset,C-Counter-2 Preset,C-Counter-3 Preset,C-Counter-4 Preset,C-Counter-5 Preset,C-Counter-6 Preset,C-Counter-7 Preset,C-Counter-8 Preset,C-Counter-0 Phase Mux Preset,C-Counter-1 Phase Mux Preset,C-Counter-2 Phase Mux Preset,C-Counter-3 Phase Mux Preset,C-Counter-4 Phase Mux Preset,C-Counter-5 Phase Mux Preset,C-Counter-6 Phase Mux Preset,C-Counter-7 Phase Mux Preset,C-Counter-8 Phase Mux Preset,Charge Pump Current,Bandwidth Control</value>
          </parameter>
          <parameter>
            <name>parameterTable_values</name>
            <value>64,1,3200.0 MHz,128,510,1,1,1,1,1,1,1,false,32,32,false,false,256,256,false,true,64,255,256,256,256,256,256,1,1,64,255,256,256,256,256,256,1,1,false,false,false,false,false,false,false,false,false,false,false,true,true,true,true,true,true,true,1,1,1,1,1,1,1,1,1,0,0,0,0,0,0,0,0,0,pll_cp_setting14,pll_bw_res_setting5</value>
          </parameter>
          <parameter>
            <name>parameter_table_hex_file</name>
            <value>seq_params_sim.hex</value>
          </parameter>
          <parameter>
            <name>pfd_clk_freq</name>
            <value>100000000</value>
          </parameter>
          <parameter>
            <name>phase_shift0</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift1</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift10</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift11</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift12</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift13</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift14</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift15</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift16</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift17</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift2</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift3</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift4</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift5</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift6</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift7</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift8</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>phase_shift9</name>
            <value>0 ps</value>
          </parameter>
          <parameter>
            <name>pll_auto_clk_sw_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_bw_sel</name>
            <value>Low</value>
          </parameter>
          <parameter>
            <name>pll_bwctrl</name>
            <value>pll_bw_res_setting5</value>
          </parameter>
          <parameter>
            <name>pll_cal_done</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_clk_loss_sw_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_clk_sw_dly</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>pll_clkin_0_src</name>
            <value>clk_0</value>
          </parameter>
          <parameter>
            <name>pll_clkin_1_src</name>
            <value>clk_0</value>
          </parameter>
          <parameter>
            <name>pll_cp_current</name>
            <value>pll_cp_setting14</value>
          </parameter>
          <parameter>
            <name>pll_defer_cal_user_mode</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>pll_dsm_out_sel</name>
            <value>1st_order</value>
          </parameter>
          <parameter>
            <name>pll_extclk_0_cnt_src</name>
            <value>pll_extclk_cnt_src_vss</value>
          </parameter>
          <parameter>
            <name>pll_extclk_1_cnt_src</name>
            <value>pll_extclk_cnt_src_vss</value>
          </parameter>
          <parameter>
            <name>pll_fbclk_mux_1</name>
            <value>pll_fbclk_mux_1_glb</value>
          </parameter>
          <parameter>
            <name>pll_fbclk_mux_2</name>
            <value>pll_fbclk_mux_2_m_cnt</value>
          </parameter>
          <parameter>
            <name>pll_fractional_cout</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>pll_fractional_division</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>pll_freqcal_en</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>pll_freqcal_req_flag</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>pll_lock_fltr_cfg</name>
            <value>100</value>
          </parameter>
          <parameter>
            <name>pll_m_cnt</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>pll_m_cnt_basic</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>pll_m_cnt_in_src</name>
            <value>c_m_cnt_in_src_ph_mux_clk</value>
          </parameter>
          <parameter>
            <name>pll_manu_clk_sw_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_output_clk_frequency</name>
            <value>3200.0 MHz</value>
          </parameter>
          <parameter>
            <name>pll_pfd_frequency</name>
            <value>50.0 MHz</value>
          </parameter>
          <parameter>
            <name>pll_ripplecap_ctrl</name>
            <value></value>
          </parameter>
          <parameter>
            <name>pll_slf_rst</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_subtype</name>
            <value>General</value>
          </parameter>
          <parameter>
            <name>pll_tclk_mux_en</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>pll_tclk_sel</name>
            <value>pll_tclk_m_src</value>
          </parameter>
          <parameter>
            <name>pll_type</name>
            <value>Agilex 5</value>
          </parameter>
          <parameter>
            <name>pll_unlock_fltr_cfg</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>pll_vco_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>pll_vco_freq_band_0</name>
            <value>pll_freq_clk0_band18</value>
          </parameter>
          <parameter>
            <name>pll_vco_freq_band_1</name>
            <value>pll_freq_clk1_band18</value>
          </parameter>
          <parameter>
            <name>pll_vcoph_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>prot_mode</name>
            <value>BASIC</value>
          </parameter>
          <parameter>
            <name>protocol_mode</name>
            <value>PROTOCOL_MODE_BASIC</value>
          </parameter>
          <parameter>
            <name>ref_clk_0_freq</name>
            <value>100000000</value>
          </parameter>
          <parameter>
            <name>ref_clk_1_freq</name>
            <value>100000000</value>
          </parameter>
          <parameter>
            <name>ref_clk_delay</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>ref_clk_n_div</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>refclk1_frequency</name>
            <value>0 MHz</value>
          </parameter>
          <parameter>
            <name>reference_clock_frequency</name>
            <value>50.0 MHz</value>
          </parameter>
          <parameter>
            <name>set_dutycycle</name>
            <value>SET_DUTYCYCLE_FRACTION</value>
          </parameter>
          <parameter>
            <name>set_fractional</name>
            <value>SET_FRACTIONAL_FRACTION</value>
          </parameter>
          <parameter>
            <name>set_freq</name>
            <value>SET_FREQ_DIVISION</value>
          </parameter>
          <parameter>
            <name>set_phase</name>
            <value>SET_PHASE_NUM_SHIFTS</value>
          </parameter>
          <parameter>
            <name>system_info_device_component</name>
            <value>A5EB013BB23BE4SCS</value>
          </parameter>
          <parameter>
            <name>system_info_device_family</name>
            <value>Agilex 5</value>
          </parameter>
          <parameter>
            <name>system_info_device_iobank_rev</name>
            <value></value>
          </parameter>
          <parameter>
            <name>system_info_device_speed_grade</name>
            <value>4</value>
          </parameter>
          <parameter>
            <name>system_part_trait_iobank_rev</name>
            <value>IO96B_REVB1</value>
          </parameter>
          <parameter>
            <name>system_part_trait_speed_grade</name>
            <value>4</value>
          </parameter>
          <parameter>
            <name>use_core_refclk</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>vco_clk_freq</name>
            <value>1000000000</value>
          </parameter>
        </parameters>
        <interconnectAssignments></interconnectAssignments>
        <className>altera_iopll</className>
        <version>21.1.0</version>
        <name>iopll_0</name>
        <uniqueName>pll_altera_iopll_2110_amd7dlq</uniqueName>
        <nonce>0</nonce>
        <incidentConnections></incidentConnections>
        <path>pll.iopll_0</path>
      </instanceData>
      <children></children>
    </node>
  </children>
</node>