<?xml version="1.0" ?>
<node xmlns:xsi="http://www.w3.org/2001/XMLSchema-instance" xmlns:xs="http://www.w3.org/2001/XMLSchema" xmlns:altera="http://www.altera.com/XMLSchema/Qsys/SystemTree">
  <instanceKey xsi:type="xs:string">EMIF_Qsys_emif_ddr4a_0</instanceKey>
  <instanceData xsi:type="data">
    <parameters></parameters>
    <interconnectAssignments></interconnectAssignments>
    <className>EMIF_Qsys_emif_ddr4a_0</className>
    <version>1.0</version>
    <name>EMIF_Qsys_emif_ddr4a_0</name>
    <uniqueName>EMIF_Qsys_emif_ddr4a_0</uniqueName>
    <nonce>0</nonce>
    <incidentConnections></incidentConnections>
  </instanceData>
  <children>
    <node>
      <instanceKey xsi:type="xs:string">EMIF_Qsys_emif_ddr4a_0</instanceKey>
      <instanceData xsi:type="data">
        <parameters>
          <parameter>
            <name>ADV_CAL_ENABLE_MARGIN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>ADV_CAL_ENABLE_REQ</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>ADV_CAL_ENABLE_WEQ</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>ANALOG_PARAM_DERIVATION_PARAM_NAME</name>
            <value></value>
          </parameter>
          <parameter>
            <name>AXI4_ADDR_WIDTH</name>
            <value>30</value>
          </parameter>
          <parameter>
            <name>CTRL_ALL_STRB_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_AUTO_PRECHARGE_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_DM_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>CTRL_ECC_AUTOCORRECT_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_ECC_INLINE_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_FIXED_PRIORITY_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_FIXED_R_PRIORITY</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>CTRL_FIXED_W_PRIORITY</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>CTRL_PERFORMANCE_PROFILE</name>
            <value>SEQ</value>
          </parameter>
          <parameter>
            <name>CTRL_PLACEMENT_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>CTRL_RD_DBI_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>CTRL_SCRAMBLER_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>CTRL_WR_DBI_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>DEBUG_PRINT_LEVEL</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>DEBUG_TOOLS_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>DIAG_EXTRA_PARAMETERS</name>
            <value></value>
          </parameter>
          <parameter>
            <name>DIAG_FORCE_SLIM_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>DIAG_HMC_ADDR_SWAP_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EMIF_INST_NAME</name>
            <value></value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_GEN_CDC</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_GEN_SIM</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_GEN_SYNTH</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_HDL_FORMAT</name>
            <value>VERILOG</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_NOC_PLL_REFCLK_FREQ_MHZ</name>
            <value>100</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_CH0_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_CH1_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_CH2_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_CH3_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_PMON_INTERNAL_JAMB_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_TG_CSR_ACCESS_MODE</name>
            <value>JTAG</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_TG_PROGRAM</name>
            <value>MEDIUM</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_TG_WIDE_IF</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ</name>
            <value>275.0</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ_AUTOSET_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>EX_DESIGN_USER_PLL_REFCLK_FREQ_MHZ</name>
            <value>100.0</value>
          </parameter>
          <parameter>
            <name>INSTANCE_ID</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>IS_HPS</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>JEDEC_OVERRIDE_TABLE_PARAM_NAME</name>
            <value>MEM_TRFCPB_NS,MEM_TCCD_NS,MEM_TCMDCKE_NS,MEM_TCKCKEH_NS,MEM_TZQCKE_NS,MEM_TESCKE_NS,MEM_RD_POSTAMBLE_CYC,MEM_WR_POSTAMBLE_CYC,MEM_TRFCAB_NS</value>
          </parameter>
          <parameter>
            <name>MEM_BANK_ADDR_WIDTH</name>
            <value>3</value>
          </parameter>
          <parameter>
            <name>MEM_CA_VREF</name>
            <value>13</value>
          </parameter>
          <parameter>
            <name>MEM_CA_WIDTH</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>MEM_CHANNEL_ADDR_NUM_BITS</name>
            <value>33</value>
          </parameter>
          <parameter>
            <name>MEM_CHANNEL_CAPACITY_GBITS</name>
            <value>8.0</value>
          </parameter>
          <parameter>
            <name>MEM_CHANNEL_CS_WIDTH</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_CHANNEL_DATA_DQ_WIDTH</name>
            <value>32</value>
          </parameter>
          <parameter>
            <name>MEM_CKE_WIDTH</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_CK_WIDTH</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_CL_CYC</name>
            <value>22</value>
          </parameter>
          <parameter>
            <name>MEM_COL_ADDR_WIDTH</name>
            <value>10</value>
          </parameter>
          <parameter>
            <name>MEM_CS_WIDTH</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_CWL_CYC</name>
            <value>18</value>
          </parameter>
          <parameter>
            <name>MEM_DIE_DENSITY_GBITS</name>
            <value>4</value>
          </parameter>
          <parameter>
            <name>MEM_DQ_PER_DQS</name>
            <value>8</value>
          </parameter>
          <parameter>
            <name>MEM_DQ_VREF</name>
            <value>20</value>
          </parameter>
          <parameter>
            <name>MEM_MINNUMREFSREQ</name>
            <value>8192.0</value>
          </parameter>
          <parameter>
            <name>MEM_NUM_CHANNELS</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_NUM_CHANNELS_PER_IO96</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_NUM_IO96</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_CA_X_CA_COMM</name>
            <value>3</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_CA_X_CA_ENABLE</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_CA_X_CK_ENABLE</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_CA_X_CS_ENABLE</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_DQ_X_IDLE</name>
            <value>off</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_DQ_X_RON</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>MEM_ODT_DQ_X_TGT_WR</name>
            <value>5</value>
          </parameter>
          <parameter>
            <name>MEM_OPERATING_FREQ_MHZ</name>
            <value>1066.667</value>
          </parameter>
          <parameter>
            <name>MEM_OPERATING_FREQ_MHZ_AUTOSET_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>MEM_PER_BANK_REF_EN</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_RD_POSTAMBLE_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>MEM_RD_PREAMBLE_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>MEM_ROW_ADDR_WIDTH</name>
            <value>15</value>
          </parameter>
          <parameter>
            <name>MEM_TCCD_NS</name>
            <value>16.0</value>
          </parameter>
          <parameter>
            <name>MEM_TCKCKEH_NS</name>
            <value>2.81</value>
          </parameter>
          <parameter>
            <name>MEM_TCKCKEL_NS</name>
            <value>5.0</value>
          </parameter>
          <parameter>
            <name>MEM_TCKEHCMD_NS</name>
            <value>7.5</value>
          </parameter>
          <parameter>
            <name>MEM_TCKELCK_NS</name>
            <value>5.0</value>
          </parameter>
          <parameter>
            <name>MEM_TCKELCMD_NS</name>
            <value>5.0</value>
          </parameter>
          <parameter>
            <name>MEM_TCKE_NS</name>
            <value>7.5</value>
          </parameter>
          <parameter>
            <name>MEM_TCMDCKE_NS</name>
            <value>2.81</value>
          </parameter>
          <parameter>
            <name>MEM_TCSCKEH_NS</name>
            <value>1.75</value>
          </parameter>
          <parameter>
            <name>MEM_TCSCKE_NS</name>
            <value>1.75</value>
          </parameter>
          <parameter>
            <name>MEM_TDQSCK_MAX_NS</name>
            <value>3.5</value>
          </parameter>
          <parameter>
            <name>MEM_TDQSCK_MIN_NS</name>
            <value>1.5</value>
          </parameter>
          <parameter>
            <name>MEM_TECH_IS_X</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>MEM_TESCKE_NS</name>
            <value>2.81</value>
          </parameter>
          <parameter>
            <name>MEM_TFAW_NS</name>
            <value>40.0</value>
          </parameter>
          <parameter>
            <name>MEM_TMRD_NS</name>
            <value>14.0</value>
          </parameter>
          <parameter>
            <name>MEM_TMRR_NS</name>
            <value>7.5</value>
          </parameter>
          <parameter>
            <name>MEM_TMRWCKEL_NS</name>
            <value>14.0</value>
          </parameter>
          <parameter>
            <name>MEM_TMRW_NS</name>
            <value>10.0</value>
          </parameter>
          <parameter>
            <name>MEM_TPPD_CYC</name>
            <value>4.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRAS_NS</name>
            <value>42.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRCD_NS</name>
            <value>18.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRC_NS</name>
            <value>63.0</value>
          </parameter>
          <parameter>
            <name>MEM_TREFI_NS</name>
            <value>3904.0</value>
          </parameter>
          <parameter>
            <name>MEM_TREFW_NS</name>
            <value>3.2E7</value>
          </parameter>
          <parameter>
            <name>MEM_TRFCAB_NS</name>
            <value>180.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRFCPB_NS</name>
            <value>90.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRPAB_NS</name>
            <value>21.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRPPB_NS</name>
            <value>18.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRRD_NS</name>
            <value>10.0</value>
          </parameter>
          <parameter>
            <name>MEM_TRTP_NS</name>
            <value>7.5</value>
          </parameter>
          <parameter>
            <name>MEM_TSR_NS</name>
            <value>15.0</value>
          </parameter>
          <parameter>
            <name>MEM_TWR_NS</name>
            <value>18.0</value>
          </parameter>
          <parameter>
            <name>MEM_TWTR_NS</name>
            <value>10.0</value>
          </parameter>
          <parameter>
            <name>MEM_TXP_NS</name>
            <value>7.5</value>
          </parameter>
          <parameter>
            <name>MEM_TXSR_NS</name>
            <value>187.5</value>
          </parameter>
          <parameter>
            <name>MEM_TZQCAL_NS</name>
            <value>1000.0</value>
          </parameter>
          <parameter>
            <name>MEM_TZQCKE_NS</name>
            <value>2.81</value>
          </parameter>
          <parameter>
            <name>MEM_TZQLAT_NS</name>
            <value>30.0</value>
          </parameter>
          <parameter>
            <name>MEM_VREF_CA_X_CA_RANGE</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>MEM_VREF_CA_X_CA_VALUE</name>
            <value>27.2</value>
          </parameter>
          <parameter>
            <name>MEM_VREF_DQ_X_RANGE</name>
            <value>1</value>
          </parameter>
          <parameter>
            <name>MEM_VREF_DQ_X_VALUE</name>
            <value>18.0</value>
          </parameter>
          <parameter>
            <name>MEM_WLS</name>
            <value>1.0</value>
          </parameter>
          <parameter>
            <name>MEM_WR_POSTAMBLE_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>NUM_IO96_IN_CHIP</name>
            <value>2</value>
          </parameter>
          <parameter>
            <name>PHY_AC_PLACEMENT</name>
            <value>BOT</value>
          </parameter>
          <parameter>
            <name>PHY_AC_TX_EQUALIZATION</name>
            <value>OFF</value>
          </parameter>
          <parameter>
            <name>PHY_CK_TX_EQUALIZATION</name>
            <value>OFF</value>
          </parameter>
          <parameter>
            <name>PHY_CS_TX_EQUALIZATION</name>
            <value>OFF</value>
          </parameter>
          <parameter>
            <name>PHY_DQ_TX_EQUALIZATION</name>
            <value>OFF</value>
          </parameter>
          <parameter>
            <name>PHY_MAINBAND_ACCESS_MODE</name>
            <value>ASYNC</value>
          </parameter>
          <parameter>
            <name>PHY_MAINBAND_ACCESS_MODE_AUTOSET_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>PHY_REFCLK_ADVANCED_SELECT_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>PHY_REFCLK_FREQ_MHZ</name>
            <value>166.6667</value>
          </parameter>
          <parameter>
            <name>PHY_REFCLK_FREQ_MHZ_AUTOSET_EN</name>
            <value>false</value>
          </parameter>
          <parameter>
            <name>PHY_SIDEBAND_ACCESS_MODE</name>
            <value>FABRIC</value>
          </parameter>
          <parameter>
            <name>PHY_SIDEBAND_ACCESS_MODE_AUTOSET_EN</name>
            <value>true</value>
          </parameter>
          <parameter>
            <name>PHY_SWIZZLE_MAP</name>
            <value>PIN_SWIZZLE_CH0_DQS0=0,1,6,7,2,4,5,3;PIN_SWIZZLE_CH0_DQS1=15,14,8,9,13,12,10,11;PIN_SWIZZLE_CH0_DQS2=18,17,21,19,20,16,22,23;PIN_SWIZZLE_CH0_DQS3=26,28,27,29,25,24,31,30;</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_AC_OUTPUT_IO_STD_TYPE</name>
            <value>LVSTL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_AC_SLEW_RATE</name>
            <value>FASTEST</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_CK_OUTPUT_IO_STD_TYPE</name>
            <value>DF_LVSTL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_CK_SLEW_RATE</name>
            <value>FASTEST</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_CS_OUTPUT_IO_STD_TYPE</name>
            <value>LVSTL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_CS_SLEW_RATE</name>
            <value>FASTEST</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_DQS_IO_STD_TYPE</name>
            <value>DF_LVSTL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_DQ_IO_STD_TYPE</name>
            <value>LVSTL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_DQ_SLEW_RATE</name>
            <value>FASTEST</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_DQ_VREF</name>
            <value>17.5</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_GPIO_IO_STD_TYPE</name>
            <value>LVCMOS</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_REFCLK_IO_STD_TYPE</name>
            <value>TRUE_DIFF</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_S_AC_OUTPUT_OHM</name>
            <value>SERIES_40_OHM_CAL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_S_CK_OUTPUT_OHM</name>
            <value>SERIES_40_OHM_CAL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_S_CS_OUTPUT_OHM</name>
            <value>SERIES_40_OHM_CAL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_S_DQ_OUTPUT_OHM</name>
            <value>SERIES_40_OHM_CAL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_T_DQ_INPUT_OHM</name>
            <value>RT_50_OHM_CAL</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_T_GPIO_INPUT_OHM</name>
            <value>RT_OFF</value>
          </parameter>
          <parameter>
            <name>PHY_TERM_X_R_T_REFCLK_INPUT_OHM</name>
            <value>RT_DIFF</value>
          </parameter>
          <parameter>
            <name>PLACEMENT_SCHEMES</name>
            <value>LPDDR4_X32_BOT</value>
          </parameter>
          <parameter>
            <name>S0_AXID_WIDTH</name>
            <value>7</value>
          </parameter>
          <parameter>
            <name>S1_AXID_WIDTH</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>S2_AXID_WIDTH</name>
            <value>7</value>
          </parameter>
          <parameter>
            <name>S3_AXID_WIDTH</name>
            <value>6</value>
          </parameter>
          <parameter>
            <name>SYSINFO_BOARD</name>
            <value>default</value>
          </parameter>
          <parameter>
            <name>SYSINFO_BOARD_TRAIT</name>
            <value></value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE</name>
            <value>A5EB013BB23BE4SCS</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_BASE_DIE</name>
            <value>SM4REVB</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_DIE_REVISIONS</name>
            <value>MAIN_SM4_REVB</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_FAMILY</name>
            <value>Agilex 5</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_GROUP</name>
            <value>B</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_IOBANK_REVISION</name>
            <value>IO96B_REVB1</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_POWER_MODEL</name>
            <value>STANDARD_POWER_FIXED</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_SPEEDGRADE</name>
            <value>4</value>
          </parameter>
          <parameter>
            <name>SYSINFO_DEVICE_TEMPERATURE_GRADE</name>
            <value>EXTENDED</value>
          </parameter>
          <parameter>
            <name>SYSINFO_SUPPORTS_VID</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_R2R_DIFFCS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_R2R_SAMECS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_R2W_DIFFCS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_R2W_SAMECS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_W2R_DIFFCS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_W2R_SAMECS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_W2W_DIFFCS_CYC</name>
            <value>0</value>
          </parameter>
          <parameter>
            <name>TURNAROUND_W2W_SAMECS_CYC</name>
            <value>0</value>
          </parameter>
        </parameters>
        <interconnectAssignments></interconnectAssignments>
        <className>emif_io96b_lpddr4</className>
        <version>4.2.0</version>
        <name>EMIF_Qsys_emif_ddr4a_0</name>
        <uniqueName>EMIF_Qsys_emif_ddr4a_0_emif_io96b_lpddr4_420_ddgvvei</uniqueName>
        <nonce>0</nonce>
        <incidentConnections></incidentConnections>
        <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0</path>
      </instanceData>
      <children>
        <node>
          <instanceKey xsi:type="xs:string">cal_0</instanceKey>
          <instanceData xsi:type="data">
            <parameters>
              <parameter>
                <name>ALL_INTFS</name>
                <value>true</value>
              </parameter>
              <parameter>
                <name>BANK_ADJACENT_PAIR_ID</name>
                <value>0</value>
              </parameter>
              <parameter>
                <name>DEBUG_TOOLS_EN</name>
                <value>false</value>
              </parameter>
              <parameter>
                <name>INSTANCE_ID</name>
                <value>1</value>
              </parameter>
              <parameter>
                <name>INSTANCE_NAME</name>
                <value>cal_0</value>
              </parameter>
              <parameter>
                <name>IS_HPS</name>
                <value>false</value>
              </parameter>
              <parameter>
                <name>IS_PART_OF_BANK_ADJACENT_PAIR</name>
                <value>false</value>
              </parameter>
              <parameter>
                <name>LOCKSTEP_ENABLE</name>
                <value>false</value>
              </parameter>
              <parameter>
                <name>NUM_CALBUS_PERIPHS</name>
                <value>1</value>
              </parameter>
              <parameter>
                <name>NUM_CALBUS_PLLS</name>
                <value>0</value>
              </parameter>
              <parameter>
                <name>PORT_M_AXIL_ENABLE</name>
                <value>false</value>
              </parameter>
              <parameter>
                <name>PORT_S_AXIL_MODE</name>
                <value>FABRIC</value>
              </parameter>
              <parameter>
                <name>SYSINFO_BOARD</name>
                <value>default</value>
              </parameter>
              <parameter>
                <name>SYSINFO_BOARD_TRAIT</name>
                <value></value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE</name>
                <value>A5EB013BB23BE4SCS</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_BASE_DIE</name>
                <value>SM4REVB</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_DIE_REVISIONS</name>
                <value>MAIN_SM4_REVB</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_FAMILY</name>
                <value>Agilex 5</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_GROUP</name>
                <value>B</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_IOBANK_REVISION</name>
                <value>IO96B_REVB1</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_POWER_MODEL</name>
                <value>STANDARD_POWER_FIXED</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_SPEEDGRADE</name>
                <value>4</value>
              </parameter>
              <parameter>
                <name>SYSINFO_DEVICE_TEMPERATURE_GRADE</name>
                <value>EXTENDED</value>
              </parameter>
              <parameter>
                <name>SYSINFO_SUPPORTS_VID</name>
                <value>0</value>
              </parameter>
            </parameters>
            <interconnectAssignments></interconnectAssignments>
            <className>emif_io96b_lpddr4_emif_io96b_cal</className>
            <version>4.2.0</version>
            <name>cal_0</name>
            <uniqueName>EMIF_Qsys_emif_ddr4a_0_emif_io96b_lpddr4_emif_io96b_cal_420_ym42tby</uniqueName>
            <nonce>0</nonce>
            <incidentConnections></incidentConnections>
            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0</path>
          </instanceData>
          <children>
            <node>
              <instanceKey xsi:type="xs:string">cal_0</instanceKey>
              <instanceData xsi:type="data">
                <parameters>
                  <parameter>
                    <name>ALL_INTFS</name>
                    <value>true</value>
                  </parameter>
                  <parameter>
                    <name>BANK_ADJACENT_PAIR_ID</name>
                    <value>0</value>
                  </parameter>
                  <parameter>
                    <name>DEBUG_TOOLS_EN</name>
                    <value>false</value>
                  </parameter>
                  <parameter>
                    <name>INSTANCE_ID</name>
                    <value>1</value>
                  </parameter>
                  <parameter>
                    <name>INSTANCE_NAME</name>
                    <value>cal_0</value>
                  </parameter>
                  <parameter>
                    <name>IS_HPS</name>
                    <value>false</value>
                  </parameter>
                  <parameter>
                    <name>IS_PART_OF_BANK_ADJACENT_PAIR</name>
                    <value>false</value>
                  </parameter>
                  <parameter>
                    <name>LOCKSTEP_ENABLE</name>
                    <value>false</value>
                  </parameter>
                  <parameter>
                    <name>NUM_CALBUS_PERIPHS</name>
                    <value>1</value>
                  </parameter>
                  <parameter>
                    <name>NUM_CALBUS_PLLS</name>
                    <value>0</value>
                  </parameter>
                  <parameter>
                    <name>PORT_M_AXIL_ENABLE</name>
                    <value>false</value>
                  </parameter>
                  <parameter>
                    <name>PORT_S_AXIL_MODE</name>
                    <value>FABRIC</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_BOARD</name>
                    <value>default</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_BOARD_TRAIT</name>
                    <value></value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE</name>
                    <value>A5EB013BB23BE4SCS</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_BASE_DIE</name>
                    <value>SM4REVB</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_DIE_REVISIONS</name>
                    <value>MAIN_SM4_REVB</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_FAMILY</name>
                    <value>Agilex 5</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_GROUP</name>
                    <value>B</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_IOBANK_REVISION</name>
                    <value>IO96B_REVB1</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_POWER_MODEL</name>
                    <value>STANDARD_POWER_FIXED</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_SPEEDGRADE</name>
                    <value>4</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_DEVICE_TEMPERATURE_GRADE</name>
                    <value>EXTENDED</value>
                  </parameter>
                  <parameter>
                    <name>SYSINFO_SUPPORTS_VID</name>
                    <value>0</value>
                  </parameter>
                </parameters>
                <interconnectAssignments></interconnectAssignments>
                <className>emif_io96b_cal</className>
                <version>2.3.2</version>
                <name>cal_0</name>
                <uniqueName>EMIF_Qsys_emif_ddr4a_0_emif_io96b_cal_232_l4guqcq</uniqueName>
                <nonce>0</nonce>
                <incidentConnections></incidentConnections>
                <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0</path>
              </instanceData>
              <children>
                <node>
                  <instanceKey xsi:type="xs:string">jamb</instanceKey>
                  <instanceData xsi:type="data">
                    <parameters>
                      <parameter>
                        <name>AUTO_BOARD</name>
                        <value></value>
                      </parameter>
                      <parameter>
                        <name>AUTO_DEVICE</name>
                        <value></value>
                      </parameter>
                      <parameter>
                        <name>AUTO_DEVICE_FAMILY</name>
                        <value></value>
                      </parameter>
                      <parameter>
                        <name>AUTO_DEVICE_SPEEDGRADE</name>
                        <value></value>
                      </parameter>
                      <parameter>
                        <name>COMPONENT_CLOCK</name>
                        <value>0</value>
                      </parameter>
                      <parameter>
                        <name>FAST_VER</name>
                        <value>0</value>
                      </parameter>
                      <parameter>
                        <name>FIFO_DEPTHS</name>
                        <value>2</value>
                      </parameter>
                      <parameter>
                        <name>PLI_PORT</name>
                        <value>50000</value>
                      </parameter>
                      <parameter>
                        <name>USE_PLI</name>
                        <value>0</value>
                      </parameter>
                    </parameters>
                    <interconnectAssignments></interconnectAssignments>
                    <className>emif_io96b_cal_alt_mem_if_jtag_master</className>
                    <version>2.3.2</version>
                    <name>jamb</name>
                    <uniqueName>EMIF_Qsys_emif_ddr4a_0_emif_io96b_cal_alt_mem_if_jtag_master_232_ch65psa</uniqueName>
                    <nonce>0</nonce>
                    <incidentConnections></incidentConnections>
                    <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb</path>
                  </instanceData>
                  <children>
                    <node>
                      <instanceKey xsi:type="xs:string">jamb</instanceKey>
                      <instanceData xsi:type="data">
                        <parameters>
                          <parameter>
                            <name>COMPONENT_CLOCK</name>
                            <value>0</value>
                          </parameter>
                          <parameter>
                            <name>FAST_VER</name>
                            <value>0</value>
                          </parameter>
                          <parameter>
                            <name>FIFO_DEPTHS</name>
                            <value>2</value>
                          </parameter>
                          <parameter>
                            <name>PLI_PORT</name>
                            <value>50000</value>
                          </parameter>
                          <parameter>
                            <name>USE_PLI</name>
                            <value>0</value>
                          </parameter>
                        </parameters>
                        <interconnectAssignments></interconnectAssignments>
                        <className>alt_mem_if_jtag_master</className>
                        <version>19.1</version>
                        <name>jamb</name>
                        <uniqueName>EMIF_Qsys_emif_ddr4a_0_alt_mem_if_jtag_master_191_2xbfrbi</uniqueName>
                        <nonce>0</nonce>
                        <incidentConnections></incidentConnections>
                        <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb</path>
                      </instanceData>
                      <children>
                        <node>
                          <instanceKey xsi:type="xs:string">b2p</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>CHANNEL_WIDTH</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>CHANNEL_WIDTH_DERIVED</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>ENCODING</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_avalon_st_bytes_to_packets</className>
                            <version>19.2.2</version>
                            <name>b2p</name>
                            <uniqueName>altera_avalon_st_bytes_to_packets</uniqueName>
                            <fixedName>altera_avalon_st_bytes_to_packets</fixedName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>b2p.out_packets_stream/b2p_adapter.in</name>
                                <end>b2p_adapter/in</end>
                                <start>b2p/out_packets_stream</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/b2p.clk</name>
                                <end>b2p/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>fifo.out/b2p.in_bytes_stream</name>
                                <end>b2p/in_bytes_stream</end>
                                <start>fifo/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>b2p/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.b2p</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">b2p_adapter</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>SYNC_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inBitsPerSymbol</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>inChannelWidth</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>inErrorDescriptor</name>
                                <value></value>
                              </parameter>
                              <parameter>
                                <name>inErrorWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inMaxChannel</name>
                                <value>255</value>
                              </parameter>
                              <parameter>
                                <name>inReadyLatency</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inSymbolsPerBeat</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmpty</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmptyPort</name>
                                <value>AUTO</value>
                              </parameter>
                              <parameter>
                                <name>inUsePackets</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>inUseReady</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>outChannelWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>outMaxChannel</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>suppressHigherChannels</name>
                                <value>true</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>channel_adapter</className>
                            <version>19.2.2</version>
                            <name>b2p_adapter</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_channel_adapter_1922_rd56ufy</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>b2p.out_packets_stream/b2p_adapter.in</name>
                                <end>b2p_adapter/in</end>
                                <start>b2p/out_packets_stream</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>b2p_adapter.out/transacto.in_stream</name>
                                <end>transacto/in_stream</end>
                                <start>b2p_adapter/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/b2p_adapter.clk</name>
                                <end>b2p_adapter/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>b2p_adapter/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.b2p_adapter</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">clk_rst</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>ACTIVE_LOW_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>NUM_RESET_OUTPUTS</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>O_SYNCHRONOUS_EDGES</name>
                                <value>none</value>
                              </parameter>
                              <parameter>
                                <name>SYNCHRONOUS_EDGES</name>
                                <value>none</value>
                              </parameter>
                              <parameter>
                                <name>SYNC_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_reset_bridge</className>
                            <version>19.2.0</version>
                            <name>clk_rst</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_altera_reset_bridge_1920_xf2264i</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>rst_controller/reset_in0</end>
                                <start>clk_rst/out_reset</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.clk_rst</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">clk_src</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>DERIVED_CLOCK_RATE</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>EXPLICIT_CLOCK_RATE</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>NUM_CLOCK_OUTPUTS</name>
                                <value>1</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_clock_bridge</className>
                            <version>19.2.0</version>
                            <name>clk_src</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_altera_clock_bridge_1920_njakcna</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/b2p.clk</name>
                                <end>b2p/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/b2p_adapter.clk</name>
                                <end>b2p_adapter/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/fifo.clk</name>
                                <end>fifo/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/jtag_phy_embedded_in_jtag_master.clock</name>
                                <end>jtag_phy_embedded_in_jtag_master/clock</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/p2b.clk</name>
                                <end>p2b/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/p2b_adapter.clk</name>
                                <end>p2b_adapter/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <end>rst_controller/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/timing_adt.clk</name>
                                <end>timing_adt/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/transacto.clk</name>
                                <end>transacto/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.clk_src</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">fifo</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>BITS_PER_SYMBOL</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>CHANNEL_WIDTH</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>EMPTY_LATENCY</name>
                                <value>3</value>
                              </parameter>
                              <parameter>
                                <name>EMPTY_WIDTH</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>ENABLE_EXPLICIT_MAXCHANNEL</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>ERROR_WIDTH</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>EXPLICIT_MAXCHANNEL</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>FIFO_DEPTH</name>
                                <value>64</value>
                              </parameter>
                              <parameter>
                                <name>MEM_TYPE</name>
                                <value>M20K</value>
                              </parameter>
                              <parameter>
                                <name>SYMBOLS_PER_BEAT</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>SYNC_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_ALMOST_EMPTY_IF</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_ALMOST_FULL_IF</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_FILL_LEVEL</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_MEMORY_BLOCKS</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>USE_PACKETS</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_STORE_FORWARD</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_avalon_sc_fifo</className>
                            <version>19.3.2</version>
                            <name>fifo</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_altera_avalon_sc_fifo_1932_onpcouq</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/fifo.clk</name>
                                <end>fifo/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>fifo.out/b2p.in_bytes_stream</name>
                                <end>b2p/in_bytes_stream</end>
                                <start>fifo/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>fifo/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>timing_adt.out/fifo.in</name>
                                <end>fifo/in</end>
                                <start>timing_adt/out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.fifo</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">jtag_phy_embedded_in_jtag_master</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>COMPONENT_CLOCK</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>DOWNSTREAM_FIFO_SIZE</name>
                                <value>64</value>
                              </parameter>
                              <parameter>
                                <name>EXPORT_JTAG</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>FABRIC</name>
                                <value>2.0</value>
                              </parameter>
                              <parameter>
                                <name>MGMT_CHANNEL_WIDTH</name>
                                <value>-1</value>
                              </parameter>
                              <parameter>
                                <name>PLI_PORT</name>
                                <value>50000</value>
                              </parameter>
                              <parameter>
                                <name>PURPOSE</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>UPSTREAM_FIFO_SIZE</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_DOWNSTREAM_READY</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_PLI</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_jtag_dc_streaming</className>
                            <version>19.1</version>
                            <name>jtag_phy_embedded_in_jtag_master</name>
                            <uniqueName>altera_avalon_st_jtag_interface</uniqueName>
                            <fixedName>altera_avalon_st_jtag_interface</fixedName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/jtag_phy_embedded_in_jtag_master.clock</name>
                                <end>jtag_phy_embedded_in_jtag_master/clock</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>jtag_phy_embedded_in_jtag_master.src/timing_adt.in</name>
                                <end>timing_adt/in</end>
                                <start>jtag_phy_embedded_in_jtag_master/src</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>p2b.out_bytes_stream/jtag_phy_embedded_in_jtag_master.sink</name>
                                <end>jtag_phy_embedded_in_jtag_master/sink</end>
                                <start>p2b/out_bytes_stream</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>jtag_phy_embedded_in_jtag_master/clock_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.jtag_phy_embedded_in_jtag_master</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">p2b</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>CHANNEL_WIDTH</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>CHANNEL_WIDTH_DERIVED</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>ENCODING</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_avalon_st_packets_to_bytes</className>
                            <version>19.2.2</version>
                            <name>p2b</name>
                            <uniqueName>altera_avalon_st_packets_to_bytes</uniqueName>
                            <fixedName>altera_avalon_st_packets_to_bytes</fixedName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/p2b.clk</name>
                                <end>p2b/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>p2b.out_bytes_stream/jtag_phy_embedded_in_jtag_master.sink</name>
                                <end>jtag_phy_embedded_in_jtag_master/sink</end>
                                <start>p2b/out_bytes_stream</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>p2b_adapter.out/p2b.in_packets_stream</name>
                                <end>p2b/in_packets_stream</end>
                                <start>p2b_adapter/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>p2b/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.p2b</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">p2b_adapter</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>SYNC_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inBitsPerSymbol</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>inChannelWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inErrorDescriptor</name>
                                <value></value>
                              </parameter>
                              <parameter>
                                <name>inErrorWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inMaxChannel</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inReadyLatency</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inSymbolsPerBeat</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmpty</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmptyPort</name>
                                <value>AUTO</value>
                              </parameter>
                              <parameter>
                                <name>inUsePackets</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>inUseReady</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>outChannelWidth</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>outMaxChannel</name>
                                <value>255</value>
                              </parameter>
                              <parameter>
                                <name>suppressHigherChannels</name>
                                <value>true</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>channel_adapter</className>
                            <version>19.2.2</version>
                            <name>p2b_adapter</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_channel_adapter_1922_5vp3d5a</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/p2b_adapter.clk</name>
                                <end>p2b_adapter/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>p2b_adapter.out/p2b.in_packets_stream</name>
                                <end>p2b/in_packets_stream</end>
                                <start>p2b_adapter/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>p2b_adapter/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>transacto.out_stream/p2b_adapter.in</name>
                                <end>p2b_adapter/in</end>
                                <start>transacto/out_stream</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.p2b_adapter</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">rst_controller</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>ADAPT_RESET_REQUEST</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>MIN_RST_ASSERTION_TIME</name>
                                <value>3</value>
                              </parameter>
                              <parameter>
                                <name>NUM_RESET_INPUTS</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>OUTPUT_RESET_SYNC_EDGES</name>
                                <value>deassert</value>
                              </parameter>
                              <parameter>
                                <name>RESET_REQUEST_PRESENT</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>RESET_REQ_EARLY_DSRT_TIME</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>RESET_REQ_WAIT_TIME</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>SYNC_DEPTH</name>
                                <value>2</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN0</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN1</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN10</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN11</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN12</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN13</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN14</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN15</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN2</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN3</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN4</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN5</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN6</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN7</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN8</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_IN9</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>USE_RESET_REQUEST_INPUT</name>
                                <value>0</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_reset_controller</className>
                            <version>19.2.4</version>
                            <name>rst_controller</name>
                            <uniqueName>altera_reset_controller</uniqueName>
                            <fixedName>altera_reset_controller</fixedName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>rst_controller/reset_in0</end>
                                <start>clk_rst/out_reset</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <end>rst_controller/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>b2p/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>b2p_adapter/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>fifo/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>jtag_phy_embedded_in_jtag_master/clock_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>p2b/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>p2b_adapter/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>timing_adt/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>transacto/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.rst_controller</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">timing_adt</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>FAMILY</name>
                                <value>Unknown</value>
                              </parameter>
                              <parameter>
                                <name>FIFO_MEM_TYPE</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>SYNC_RESET</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inBitsPerSymbol</name>
                                <value>8</value>
                              </parameter>
                              <parameter>
                                <name>inChannelWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inErrorDescriptor</name>
                                <value></value>
                              </parameter>
                              <parameter>
                                <name>inErrorWidth</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inMaxChannel</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inReadyLatency</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>inSymbolsPerBeat</name>
                                <value>1</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmpty</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>inUseEmptyPort</name>
                                <value>NO</value>
                              </parameter>
                              <parameter>
                                <name>inUsePackets</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>inUseReady</name>
                                <value>false</value>
                              </parameter>
                              <parameter>
                                <name>inUseValid</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>outReadyLatency</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>outUseReady</name>
                                <value>true</value>
                              </parameter>
                              <parameter>
                                <name>outUseValid</name>
                                <value>true</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>timing_adapter</className>
                            <version>19.5.0</version>
                            <name>timing_adt</name>
                            <uniqueName>EMIF_Qsys_emif_ddr4a_0_timing_adapter_1950_bbjt6kq</uniqueName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/timing_adt.clk</name>
                                <end>timing_adt/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>jtag_phy_embedded_in_jtag_master.src/timing_adt.in</name>
                                <end>timing_adt/in</end>
                                <start>jtag_phy_embedded_in_jtag_master/src</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>timing_adt/reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>timing_adt.out/fifo.in</name>
                                <end>fifo/in</end>
                                <start>timing_adt/out</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.timing_adt</path>
                          </instanceData>
                          <children></children>
                        </node>
                        <node>
                          <instanceKey xsi:type="xs:string">transacto</instanceKey>
                          <instanceData xsi:type="data">
                            <parameters>
                              <parameter>
                                <name>EXPORT_MASTER_SIGNALS</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>FAST_VER</name>
                                <value>0</value>
                              </parameter>
                              <parameter>
                                <name>FIFO_DEPTHS</name>
                                <value>2</value>
                              </parameter>
                              <parameter>
                                <name>FIFO_WIDTHU</name>
                                <value>1</value>
                              </parameter>
                            </parameters>
                            <interconnectAssignments></interconnectAssignments>
                            <className>altera_avalon_packets_to_master</className>
                            <version>19.2.2</version>
                            <name>transacto</name>
                            <uniqueName>altera_avalon_packets_to_master</uniqueName>
                            <fixedName>altera_avalon_packets_to_master</fixedName>
                            <nonce>0</nonce>
                            <incidentConnections>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>b2p_adapter.out/transacto.in_stream</name>
                                <end>transacto/in_stream</end>
                                <start>b2p_adapter/out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>clockRateSysInfo</name>
                                    <value></value>
                                  </parameter>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>clock</className>
                                <version>26.1</version>
                                <name>clk_src.out_clk/transacto.clk</name>
                                <end>transacto/clk</end>
                                <start>clk_src/out_clk</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>resetDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockDomainSysInfo</name>
                                    <value>-1</value>
                                  </parameter>
                                  <parameter>
                                    <name>clockResetSysInfo</name>
                                    <value></value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>reset</className>
                                <version>26.1</version>
                                <end>transacto/clk_reset</end>
                                <start>rst_controller/reset_out</start>
                              </incidentConnection>
                              <incidentConnection>
                                <parameters>
                                  <parameter>
                                    <name>qsys_mm.piplineType</name>
                                    <value>PIPELINE_STAGE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.insertDefaultSlave</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableOutOfOrderSupport</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableInstrumentation</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.clockCrossingAdapter</name>
                                    <value>AUTO</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.widthAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectResetSource</name>
                                    <value>DEFAULT</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.burstAdapterImplementation</name>
                                    <value>GENERIC_CONVERTER</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.optimizeRdFifoSize</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.responseFifoType</name>
                                    <value>REGISTER_BASED</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.maxAdditionalLatency</name>
                                    <value>1</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.splitCommandsFor4KBoundary</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.syncResets</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.fifoDepth</name>
                                    <value>8</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableAllPipelines</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.enableEccProtection</name>
                                    <value>FALSE</value>
                                  </parameter>
                                  <parameter>
                                    <name>qsys_mm.interconnectType</name>
                                    <value>STANDARD</value>
                                  </parameter>
                                </parameters>
                                <interconnectAssignments></interconnectAssignments>
                                <className>avalon_streaming</className>
                                <version>26.1</version>
                                <name>transacto.out_stream/p2b_adapter.in</name>
                                <end>p2b_adapter/in</end>
                                <start>transacto/out_stream</start>
                              </incidentConnection>
                            </incidentConnections>
                            <path>EMIF_Qsys_emif_ddr4a_0.EMIF_Qsys_emif_ddr4a_0.cal_0.cal_0.jamb.jamb.transacto</path>
                          </instanceData>
                          <children></children>
                        </node>
                      </children>
                    </node>
                  </children>
                </node>
              </children>
            </node>
          </children>
        </node>
      </children>
    </node>
  </children>
</node>