<?xml version="1.0" ?>
<!--Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and any partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, the Altera Quartus Prime License Agreement,
the Altera FPGA IP License Agreement, or other applicable license
agreement, including, without limitation, that your use is for
the sole purpose of programming logic devices manufactured by
Altera and sold by Altera or its authorized distributors.-->
<ipxact:component xmlns:altera="http://www.altera.com/XMLSchema/IPXact2014/extensions" xmlns:ipxact="http://www.accellera.org/XMLSchema/IPXACT/1685-2014">
  <ipxact:vendor>Altera</ipxact:vendor>
  <ipxact:library>audio_pll</ipxact:library>
  <ipxact:name>iopll_0</ipxact:name>
  <ipxact:version>21.1.0</ipxact:version>
  <ipxact:busInterfaces>
    <ipxact:busInterface>
      <ipxact:name>refclk</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="clock" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="clock" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>refclk</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>50000000</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>locked</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>export</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>locked</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>reset</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="reset" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="reset" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>rst</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>input</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>outclk0</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="clock" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="clock" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>outclk_0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedDirectClock" type="string">
          <ipxact:name>associatedDirectClock</ipxact:name>
          <ipxact:displayName>Associated direct clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>12288136</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="clockRateKnown" type="bit">
          <ipxact:name>clockRateKnown</ipxact:name>
          <ipxact:displayName>Clock rate known</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="ui.blockdiagram.direction" type="string">
              <ipxact:name>ui.blockdiagram.direction</ipxact:name>
              <ipxact:value>output</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
  </ipxact:busInterfaces>
  <ipxact:model>
    <ipxact:views>
      <ipxact:view>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:envIdentifier>:quartus.altera.com:</ipxact:envIdentifier>
        <ipxact:componentInstantiationRef>QUARTUS_SYNTH</ipxact:componentInstantiationRef>
      </ipxact:view>
    </ipxact:views>
    <ipxact:instantiations>
      <ipxact:componentInstantiation>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:moduleName>altera_iopll</ipxact:moduleName>
        <ipxact:fileSetRef>
          <ipxact:localName>QUARTUS_SYNTH</ipxact:localName>
        </ipxact:fileSetRef>
      </ipxact:componentInstantiation>
    </ipxact:instantiations>
    <ipxact:ports>
      <ipxact:port>
        <ipxact:name>refclk</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>locked</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>rst</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>outclk_0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
    </ipxact:ports>
  </ipxact:model>
  <ipxact:vendorExtensions>
    <altera:entity_info>
      <ipxact:vendor>Altera</ipxact:vendor>
      <ipxact:library>audio_pll</ipxact:library>
      <ipxact:name>altera_iopll</ipxact:name>
      <ipxact:version>21.1.0</ipxact:version>
    </altera:entity_info>
    <altera:altera_module_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="gui_debug_mode" type="bit">
          <ipxact:name>gui_debug_mode</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_skip_sdc_generation" type="bit">
          <ipxact:name>gui_skip_sdc_generation</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_include_iossm" type="bit">
          <ipxact:name>gui_include_iossm</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cal_code_hex_file" type="string">
          <ipxact:name>gui_cal_code_hex_file</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>iossm.hex</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_parameter_table_hex_file" type="string">
          <ipxact:name>gui_parameter_table_hex_file</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>seq_params_sim.hex</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_tclk_mux_en" type="bit">
          <ipxact:name>gui_pll_tclk_mux_en</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_tclk_sel" type="string">
          <ipxact:name>gui_pll_tclk_sel</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>pll_tclk_m_src</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_vco_freq_band_0" type="string">
          <ipxact:name>gui_pll_vco_freq_band_0</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>pll_freq_clk0_band18</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_vco_freq_band_1" type="string">
          <ipxact:name>gui_pll_vco_freq_band_1</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>pll_freq_clk1_band18</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_freqcal_en" type="bit">
          <ipxact:name>gui_pll_freqcal_en</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_freqcal_req_flag" type="bit">
          <ipxact:name>gui_pll_freqcal_req_flag</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cal_converge" type="bit">
          <ipxact:name>gui_cal_converge</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cal_error" type="string">
          <ipxact:name>gui_cal_error</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>cal_clean</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_cal_done" type="bit">
          <ipxact:name>gui_pll_cal_done</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_type" type="string">
          <ipxact:name>gui_pll_type</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>S10_Physical</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_m_cnt_in_src" type="string">
          <ipxact:name>gui_pll_m_cnt_in_src</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src0" type="string">
          <ipxact:name>gui_c_cnt_in_src0</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src1" type="string">
          <ipxact:name>gui_c_cnt_in_src1</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src2" type="string">
          <ipxact:name>gui_c_cnt_in_src2</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src3" type="string">
          <ipxact:name>gui_c_cnt_in_src3</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src4" type="string">
          <ipxact:name>gui_c_cnt_in_src4</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src5" type="string">
          <ipxact:name>gui_c_cnt_in_src5</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src6" type="string">
          <ipxact:name>gui_c_cnt_in_src6</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src7" type="string">
          <ipxact:name>gui_c_cnt_in_src7</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_c_cnt_in_src8" type="string">
          <ipxact:name>gui_c_cnt_in_src8</ipxact:name>
          <ipxact:displayName></ipxact:displayName>
          <ipxact:value>c_m_cnt_in_src_ph_mux_clk</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_info_device_family" type="string">
          <ipxact:name>system_info_device_family</ipxact:name>
          <ipxact:displayName>Device Family</ipxact:displayName>
          <ipxact:value>Agilex 5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_info_device_component" type="string">
          <ipxact:name>system_info_device_component</ipxact:name>
          <ipxact:displayName>Component</ipxact:displayName>
          <ipxact:value>A5EB013BB23BE4SCS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_info_device_iobank_rev" type="string">
          <ipxact:name>system_info_device_iobank_rev</ipxact:name>
          <ipxact:displayName>IO Bank Revision</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_part_trait_speed_grade" type="string">
          <ipxact:name>system_part_trait_speed_grade</ipxact:name>
          <ipxact:displayName>Speed Grade Trait</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_part_trait_iobank_rev" type="string">
          <ipxact:name>system_part_trait_iobank_rev</ipxact:name>
          <ipxact:displayName>IO Bank Revision Trait</ipxact:displayName>
          <ipxact:value>IO96B_REVB1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="system_info_device_speed_grade" type="string">
          <ipxact:name>system_info_device_speed_grade</ipxact:name>
          <ipxact:displayName>Speed Grade</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_usr_device_speed_grade" type="string">
          <ipxact:name>gui_usr_device_speed_grade</ipxact:name>
          <ipxact:displayName>Speed Grade</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_reconf" type="bit">
          <ipxact:name>gui_en_reconf</ipxact:name>
          <ipxact:displayName>Enable dynamic reconfiguration of PLL</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_hvio_reconf" type="bit">
          <ipxact:name>gui_en_hvio_reconf</ipxact:name>
          <ipxact:displayName>Enable dynamic reconfiguration of PLL</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_iossm_reconf" type="bit">
          <ipxact:name>gui_en_iossm_reconf</ipxact:name>
          <ipxact:displayName>Enable dynamic reconfiguration of PLL using Calibration IP</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_user_base_address" type="int">
          <ipxact:name>gui_user_base_address</ipxact:name>
          <ipxact:displayName>User base address of PLL for dynamic reconfiguration (0..255)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_dps_ports" type="bit">
          <ipxact:name>gui_en_dps_ports</ipxact:name>
          <ipxact:displayName>Enable access to dynamic phase shift ports</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_mode" type="string">
          <ipxact:name>gui_pll_mode</ipxact:name>
          <ipxact:displayName>PLL Mode</ipxact:displayName>
          <ipxact:value>Integer-N PLL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_location_type" type="string">
          <ipxact:name>gui_location_type</ipxact:name>
          <ipxact:displayName>IOPLL Type</ipxact:displayName>
          <ipxact:value>I/O Bank</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_logical" type="bit">
          <ipxact:name>gui_use_logical</ipxact:name>
          <ipxact:displayName>Use logical PLL</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_reference_clock_frequency" type="real">
          <ipxact:name>gui_reference_clock_frequency</ipxact:name>
          <ipxact:displayName>Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_reference_clock_frequency_ps" type="real">
          <ipxact:name>gui_reference_clock_frequency_ps</ipxact:name>
          <ipxact:displayName>Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>20000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_coreclk" type="bit">
          <ipxact:name>gui_use_coreclk</ipxact:name>
          <ipxact:displayName>Refclk source is global clock</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_refclk_might_change" type="bit">
          <ipxact:name>gui_refclk_might_change</ipxact:name>
          <ipxact:displayName>My reference clock frequency might change</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_fractional_cout" type="int">
          <ipxact:name>gui_fractional_cout</ipxact:name>
          <ipxact:displayName>Fractional carry out</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_prot_mode" type="string">
          <ipxact:name>gui_prot_mode</ipxact:name>
          <ipxact:displayName>prot_mode</ipxact:displayName>
          <ipxact:value>UNUSED</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_dsm_out_sel" type="string">
          <ipxact:name>gui_dsm_out_sel</ipxact:name>
          <ipxact:displayName>DSM Order</ipxact:displayName>
          <ipxact:value>1st_order</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_locked" type="bit">
          <ipxact:name>gui_use_locked</ipxact:name>
          <ipxact:displayName>Enable 'locked' output port</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_set_locked_as_reset" type="bit">
          <ipxact:name>gui_set_locked_as_reset</ipxact:name>
          <ipxact:displayName>Set 'locked' as reset interface</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_adv_params" type="bit">
          <ipxact:name>gui_en_adv_params</ipxact:name>
          <ipxact:displayName>Enable physical output clock parameters</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_fractional_division" type="bit">
          <ipxact:name>gui_use_fractional_division</ipxact:name>
          <ipxact:displayName>Enable fractional division</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_bandwidth_preset" type="string">
          <ipxact:name>gui_pll_bandwidth_preset</ipxact:name>
          <ipxact:displayName>PLL Bandwidth Preset</ipxact:displayName>
          <ipxact:value>Low</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_lock_setting" type="string">
          <ipxact:name>gui_lock_setting</ipxact:name>
          <ipxact:displayName>Lock Threshold Setting</ipxact:displayName>
          <ipxact:value>Low Lock Time</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_auto_reset" type="bit">
          <ipxact:name>gui_pll_auto_reset</ipxact:name>
          <ipxact:displayName>PLL Auto Reset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_lvds_ports" type="string">
          <ipxact:name>gui_en_lvds_ports</ipxact:name>
          <ipxact:displayName>Access to PLL LVDS_CLK/LOADEN output port</ipxact:displayName>
          <ipxact:value>Disabled</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_periphery_ports" type="bit">
          <ipxact:name>gui_en_periphery_ports</ipxact:name>
          <ipxact:displayName>Enable access to I/O Bank clock ports</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_operation_mode" type="string">
          <ipxact:name>gui_operation_mode</ipxact:name>
          <ipxact:displayName>Compensation Mode</ipxact:displayName>
          <ipxact:value>direct</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_feedback_clock" type="string">
          <ipxact:name>gui_feedback_clock</ipxact:name>
          <ipxact:displayName>Feedback Clock</ipxact:displayName>
          <ipxact:value>Global Clock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_to_compensate" type="int">
          <ipxact:name>gui_clock_to_compensate</ipxact:name>
          <ipxact:displayName>Compensated Outclk</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_NDFB_modes" type="bit">
          <ipxact:name>gui_use_NDFB_modes</ipxact:name>
          <ipxact:displayName>Use Nondedicated Feedback Path</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_refclk_switch" type="bit">
          <ipxact:name>gui_refclk_switch</ipxact:name>
          <ipxact:displayName>Create a second input clock signal 'refclk1'</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_refclk1_frequency" type="real">
          <ipxact:name>gui_refclk1_frequency</ipxact:name>
          <ipxact:displayName>Second Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_phout_ports" type="bit">
          <ipxact:name>gui_en_phout_ports</ipxact:name>
          <ipxact:displayName>Enable access to PLL DPA output port</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phout_division" type="int">
          <ipxact:name>gui_phout_division</ipxact:name>
          <ipxact:displayName>PLL DPA output division</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_en_extclkout_ports" type="bit">
          <ipxact:name>gui_en_extclkout_ports</ipxact:name>
          <ipxact:displayName>Enable access to PLL external clock output port</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_number_of_clocks" type="int">
          <ipxact:name>gui_number_of_clocks</ipxact:name>
          <ipxact:displayName>Number Of Clocks</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_multiply_factor" type="int">
          <ipxact:name>gui_multiply_factor</ipxact:name>
          <ipxact:displayName>Multiply Factor (M-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_multiply_fraction" type="int">
          <ipxact:name>gui_multiply_fraction</ipxact:name>
          <ipxact:displayName>Multiply Factor (Fraction)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_slvs_refclk" type="bit">
          <ipxact:name>gui_use_slvs_refclk</ipxact:name>
          <ipxact:displayName>Use SLVS400 for the PLL reference clock</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_use_slvs_refclk1" type="bit">
          <ipxact:name>gui_use_slvs_refclk1</ipxact:name>
          <ipxact:displayName>Use SLVS400 for the second PLL reference clock</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_n" type="int">
          <ipxact:name>gui_divide_factor_n</ipxact:name>
          <ipxact:displayName>Divide Factor (N-Counter)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_frac_multiply_factor" type="longint">
          <ipxact:name>gui_frac_multiply_factor</ipxact:name>
          <ipxact:displayName>Fractional Multiply Factor (K)</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_fix_vco_frequency" type="bit">
          <ipxact:name>gui_fix_vco_frequency</ipxact:name>
          <ipxact:displayName>Specify VCO frequency</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_fixed_vco_frequency" type="real">
          <ipxact:name>gui_fixed_vco_frequency</ipxact:name>
          <ipxact:displayName>Desired VCO Frequency</ipxact:displayName>
          <ipxact:value>600.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_fixed_vco_frequency_ps" type="real">
          <ipxact:name>gui_fixed_vco_frequency_ps</ipxact:name>
          <ipxact:displayName>Desired VCO Frequency</ipxact:displayName>
          <ipxact:value>1667.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_vco_frequency" type="string">
          <ipxact:name>gui_vco_frequency</ipxact:name>
          <ipxact:displayName>Actual VCO Frequency</ipxact:displayName>
          <ipxact:value>600.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_output_counter_cascading" type="bit">
          <ipxact:name>gui_enable_output_counter_cascading</ipxact:name>
          <ipxact:displayName>Enable output counter cascading</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_mif_gen_options" type="string">
          <ipxact:name>gui_mif_gen_options</ipxact:name>
          <ipxact:displayName>MIF Generation Options</ipxact:displayName>
          <ipxact:value>Generate New MIF File</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_new_mif_file_path" type="string">
          <ipxact:name>gui_new_mif_file_path</ipxact:name>
          <ipxact:displayName>Path to New MIF file</ipxact:displayName>
          <ipxact:value>~/pll.mif</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_existing_mif_file_path" type="string">
          <ipxact:name>gui_existing_mif_file_path</ipxact:name>
          <ipxact:displayName>Path to Existing MIF file</ipxact:displayName>
          <ipxact:value>~/pll.mif</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_mif_config_name" type="string">
          <ipxact:name>gui_mif_config_name</ipxact:name>
          <ipxact:displayName>Name of Current Configuration</ipxact:displayName>
          <ipxact:value>unnamed</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_active_clk" type="bit">
          <ipxact:name>gui_active_clk</ipxact:name>
          <ipxact:displayName>Create an 'active_clk' signal to indicate the input clock in use</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clk_bad" type="bit">
          <ipxact:name>gui_clk_bad</ipxact:name>
          <ipxact:displayName>Create a 'clkbad' signal for each of the input clocks</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_switchover_mode" type="string">
          <ipxact:name>gui_switchover_mode</ipxact:name>
          <ipxact:displayName>Switchover Mode</ipxact:displayName>
          <ipxact:value>Automatic Switchover</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_switchover_delay" type="int">
          <ipxact:name>gui_switchover_delay</ipxact:name>
          <ipxact:displayName>Switchover Delay</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_cascade_out" type="bit">
          <ipxact:name>gui_enable_cascade_out</ipxact:name>
          <ipxact:displayName>Create a 'cascade_out' signal to connect to a downstream PLL</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_outclk_index" type="string">
          <ipxact:name>gui_cascade_outclk_index</ipxact:name>
          <ipxact:displayName>cascade_out source</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_cascade_in" type="bit">
          <ipxact:name>gui_enable_cascade_in</ipxact:name>
          <ipxact:displayName>Create an 'adjpllin' (cascade in) signal to connect to an upstream PLL through IO Column Cascading</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_permit_cal" type="bit">
          <ipxact:name>gui_enable_permit_cal</ipxact:name>
          <ipxact:displayName>Connect to an upstream PLL through Core Clock Network Cascading (create a permit_cal input signal)</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_upstream_out_clk" type="bit">
          <ipxact:name>gui_enable_upstream_out_clk</ipxact:name>
          <ipxact:displayName>Connect outclk to a downstream PLL through Core Clock Network Cascading</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_pll_cascading_mode" type="string">
          <ipxact:name>gui_pll_cascading_mode</ipxact:name>
          <ipxact:displayName>Connection Signal Type to Upstream PLL</ipxact:displayName>
          <ipxact:value>adjpllin</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_enable_mif_dps" type="bit">
          <ipxact:name>gui_enable_mif_dps</ipxact:name>
          <ipxact:displayName>Enable Dynamic Phase Shift for MIF streaming</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_dps_cntr" type="string">
          <ipxact:name>gui_dps_cntr</ipxact:name>
          <ipxact:displayName>DPS Counter Selection</ipxact:displayName>
          <ipxact:value>C0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_dps_num" type="int">
          <ipxact:name>gui_dps_num</ipxact:name>
          <ipxact:displayName>Number of Dynamic Phase Shifts</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_dps_dir" type="string">
          <ipxact:name>gui_dps_dir</ipxact:name>
          <ipxact:displayName>Dynamic Phase Shift Direction</ipxact:displayName>
          <ipxact:value>Positive</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_extclkout_0_source" type="string">
          <ipxact:name>gui_extclkout_0_source</ipxact:name>
          <ipxact:displayName>extclk_out[0] source</ipxact:displayName>
          <ipxact:value>C0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_extclkout_1_source" type="string">
          <ipxact:name>gui_extclkout_1_source</ipxact:name>
          <ipxact:displayName>extclk_out[1] source</ipxact:displayName>
          <ipxact:value>C0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_extclkout_source" type="string">
          <ipxact:name>gui_extclkout_source</ipxact:name>
          <ipxact:displayName>extclk_out source</ipxact:displayName>
          <ipxact:value>C0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_global" type="bit">
          <ipxact:name>gui_clock_name_global</ipxact:name>
          <ipxact:displayName>Give clocks global names</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_instantiation" type="bit">
          <ipxact:name>gui_clock_name_instantiation</ipxact:name>
          <ipxact:displayName>Use clock names as ports in instantiation</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string0" type="string">
          <ipxact:name>gui_clock_name_string0</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string1" type="string">
          <ipxact:name>gui_clock_name_string1</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string2" type="string">
          <ipxact:name>gui_clock_name_string2</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string3" type="string">
          <ipxact:name>gui_clock_name_string3</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string4" type="string">
          <ipxact:name>gui_clock_name_string4</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string5" type="string">
          <ipxact:name>gui_clock_name_string5</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string6" type="string">
          <ipxact:name>gui_clock_name_string6</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string7" type="string">
          <ipxact:name>gui_clock_name_string7</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string8" type="string">
          <ipxact:name>gui_clock_name_string8</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk8</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string9" type="string">
          <ipxact:name>gui_clock_name_string9</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk9</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string10" type="string">
          <ipxact:name>gui_clock_name_string10</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk10</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string11" type="string">
          <ipxact:name>gui_clock_name_string11</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk11</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string12" type="string">
          <ipxact:name>gui_clock_name_string12</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk12</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string13" type="string">
          <ipxact:name>gui_clock_name_string13</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk13</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string14" type="string">
          <ipxact:name>gui_clock_name_string14</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk14</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string15" type="string">
          <ipxact:name>gui_clock_name_string15</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk15</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string16" type="string">
          <ipxact:name>gui_clock_name_string16</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk16</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_clock_name_string17" type="string">
          <ipxact:name>gui_clock_name_string17</ipxact:name>
          <ipxact:displayName>Clock Name</ipxact:displayName>
          <ipxact:value>outclk17</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c0" type="int">
          <ipxact:name>gui_divide_factor_c0</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c1" type="int">
          <ipxact:name>gui_divide_factor_c1</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c2" type="int">
          <ipxact:name>gui_divide_factor_c2</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c3" type="int">
          <ipxact:name>gui_divide_factor_c3</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c4" type="int">
          <ipxact:name>gui_divide_factor_c4</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c5" type="int">
          <ipxact:name>gui_divide_factor_c5</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c6" type="int">
          <ipxact:name>gui_divide_factor_c6</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c7" type="int">
          <ipxact:name>gui_divide_factor_c7</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c8" type="int">
          <ipxact:name>gui_divide_factor_c8</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c9" type="int">
          <ipxact:name>gui_divide_factor_c9</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c10" type="int">
          <ipxact:name>gui_divide_factor_c10</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c11" type="int">
          <ipxact:name>gui_divide_factor_c11</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c12" type="int">
          <ipxact:name>gui_divide_factor_c12</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c13" type="int">
          <ipxact:name>gui_divide_factor_c13</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c14" type="int">
          <ipxact:name>gui_divide_factor_c14</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c15" type="int">
          <ipxact:name>gui_divide_factor_c15</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c16" type="int">
          <ipxact:name>gui_divide_factor_c16</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_divide_factor_c17" type="int">
          <ipxact:name>gui_divide_factor_c17</ipxact:name>
          <ipxact:displayName>Divide Factor (C-Counter)</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter0" type="bit">
          <ipxact:name>gui_cascade_counter0</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter1" type="bit">
          <ipxact:name>gui_cascade_counter1</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter2" type="bit">
          <ipxact:name>gui_cascade_counter2</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter3" type="bit">
          <ipxact:name>gui_cascade_counter3</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter4" type="bit">
          <ipxact:name>gui_cascade_counter4</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter5" type="bit">
          <ipxact:name>gui_cascade_counter5</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter6" type="bit">
          <ipxact:name>gui_cascade_counter6</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter7" type="bit">
          <ipxact:name>gui_cascade_counter7</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter8" type="bit">
          <ipxact:name>gui_cascade_counter8</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter9" type="bit">
          <ipxact:name>gui_cascade_counter9</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter10" type="bit">
          <ipxact:name>gui_cascade_counter10</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter11" type="bit">
          <ipxact:name>gui_cascade_counter11</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter12" type="bit">
          <ipxact:name>gui_cascade_counter12</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter13" type="bit">
          <ipxact:name>gui_cascade_counter13</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter14" type="bit">
          <ipxact:name>gui_cascade_counter14</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter15" type="bit">
          <ipxact:name>gui_cascade_counter15</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter16" type="bit">
          <ipxact:name>gui_cascade_counter16</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_cascade_counter17" type="bit">
          <ipxact:name>gui_cascade_counter17</ipxact:name>
          <ipxact:displayName>Make this a cascade counter</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency0" type="real">
          <ipxact:name>gui_output_clock_frequency0</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency1" type="real">
          <ipxact:name>gui_output_clock_frequency1</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>12.288</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency2" type="real">
          <ipxact:name>gui_output_clock_frequency2</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency3" type="real">
          <ipxact:name>gui_output_clock_frequency3</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency4" type="real">
          <ipxact:name>gui_output_clock_frequency4</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency5" type="real">
          <ipxact:name>gui_output_clock_frequency5</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency6" type="real">
          <ipxact:name>gui_output_clock_frequency6</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency7" type="real">
          <ipxact:name>gui_output_clock_frequency7</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency8" type="real">
          <ipxact:name>gui_output_clock_frequency8</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency9" type="real">
          <ipxact:name>gui_output_clock_frequency9</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency10" type="real">
          <ipxact:name>gui_output_clock_frequency10</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency11" type="real">
          <ipxact:name>gui_output_clock_frequency11</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency12" type="real">
          <ipxact:name>gui_output_clock_frequency12</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency13" type="real">
          <ipxact:name>gui_output_clock_frequency13</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency14" type="real">
          <ipxact:name>gui_output_clock_frequency14</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency15" type="real">
          <ipxact:name>gui_output_clock_frequency15</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency16" type="real">
          <ipxact:name>gui_output_clock_frequency16</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency17" type="real">
          <ipxact:name>gui_output_clock_frequency17</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps0" type="real">
          <ipxact:name>gui_output_clock_frequency_ps0</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>20000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps1" type="real">
          <ipxact:name>gui_output_clock_frequency_ps1</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>81380.208</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps2" type="real">
          <ipxact:name>gui_output_clock_frequency_ps2</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps3" type="real">
          <ipxact:name>gui_output_clock_frequency_ps3</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps4" type="real">
          <ipxact:name>gui_output_clock_frequency_ps4</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps5" type="real">
          <ipxact:name>gui_output_clock_frequency_ps5</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps6" type="real">
          <ipxact:name>gui_output_clock_frequency_ps6</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps7" type="real">
          <ipxact:name>gui_output_clock_frequency_ps7</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps8" type="real">
          <ipxact:name>gui_output_clock_frequency_ps8</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps9" type="real">
          <ipxact:name>gui_output_clock_frequency_ps9</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps10" type="real">
          <ipxact:name>gui_output_clock_frequency_ps10</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps11" type="real">
          <ipxact:name>gui_output_clock_frequency_ps11</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps12" type="real">
          <ipxact:name>gui_output_clock_frequency_ps12</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps13" type="real">
          <ipxact:name>gui_output_clock_frequency_ps13</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps14" type="real">
          <ipxact:name>gui_output_clock_frequency_ps14</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps15" type="real">
          <ipxact:name>gui_output_clock_frequency_ps15</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps16" type="real">
          <ipxact:name>gui_output_clock_frequency_ps16</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_output_clock_frequency_ps17" type="real">
          <ipxact:name>gui_output_clock_frequency_ps17</ipxact:name>
          <ipxact:displayName>Desired Frequency</ipxact:displayName>
          <ipxact:value>10000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units0" type="string">
          <ipxact:name>gui_ps_units0</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units1" type="string">
          <ipxact:name>gui_ps_units1</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units2" type="string">
          <ipxact:name>gui_ps_units2</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units3" type="string">
          <ipxact:name>gui_ps_units3</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units4" type="string">
          <ipxact:name>gui_ps_units4</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units5" type="string">
          <ipxact:name>gui_ps_units5</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units6" type="string">
          <ipxact:name>gui_ps_units6</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units7" type="string">
          <ipxact:name>gui_ps_units7</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units8" type="string">
          <ipxact:name>gui_ps_units8</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units9" type="string">
          <ipxact:name>gui_ps_units9</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units10" type="string">
          <ipxact:name>gui_ps_units10</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units11" type="string">
          <ipxact:name>gui_ps_units11</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units12" type="string">
          <ipxact:name>gui_ps_units12</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units13" type="string">
          <ipxact:name>gui_ps_units13</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units14" type="string">
          <ipxact:name>gui_ps_units14</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units15" type="string">
          <ipxact:name>gui_ps_units15</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units16" type="string">
          <ipxact:name>gui_ps_units16</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_ps_units17" type="string">
          <ipxact:name>gui_ps_units17</ipxact:name>
          <ipxact:displayName>Phase Shift Units</ipxact:displayName>
          <ipxact:value>ps</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift0" type="real">
          <ipxact:name>gui_phase_shift0</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift1" type="real">
          <ipxact:name>gui_phase_shift1</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift2" type="real">
          <ipxact:name>gui_phase_shift2</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift3" type="real">
          <ipxact:name>gui_phase_shift3</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift4" type="real">
          <ipxact:name>gui_phase_shift4</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift5" type="real">
          <ipxact:name>gui_phase_shift5</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift6" type="real">
          <ipxact:name>gui_phase_shift6</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift7" type="real">
          <ipxact:name>gui_phase_shift7</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift8" type="real">
          <ipxact:name>gui_phase_shift8</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift9" type="real">
          <ipxact:name>gui_phase_shift9</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift10" type="real">
          <ipxact:name>gui_phase_shift10</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift11" type="real">
          <ipxact:name>gui_phase_shift11</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift12" type="real">
          <ipxact:name>gui_phase_shift12</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift13" type="real">
          <ipxact:name>gui_phase_shift13</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift14" type="real">
          <ipxact:name>gui_phase_shift14</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift15" type="real">
          <ipxact:name>gui_phase_shift15</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift16" type="real">
          <ipxact:name>gui_phase_shift16</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift17" type="real">
          <ipxact:name>gui_phase_shift17</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg0" type="real">
          <ipxact:name>gui_phase_shift_deg0</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg1" type="real">
          <ipxact:name>gui_phase_shift_deg1</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg2" type="real">
          <ipxact:name>gui_phase_shift_deg2</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg3" type="real">
          <ipxact:name>gui_phase_shift_deg3</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg4" type="real">
          <ipxact:name>gui_phase_shift_deg4</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg5" type="real">
          <ipxact:name>gui_phase_shift_deg5</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg6" type="real">
          <ipxact:name>gui_phase_shift_deg6</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg7" type="real">
          <ipxact:name>gui_phase_shift_deg7</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg8" type="real">
          <ipxact:name>gui_phase_shift_deg8</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg9" type="real">
          <ipxact:name>gui_phase_shift_deg9</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg10" type="real">
          <ipxact:name>gui_phase_shift_deg10</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg11" type="real">
          <ipxact:name>gui_phase_shift_deg11</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg12" type="real">
          <ipxact:name>gui_phase_shift_deg12</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg13" type="real">
          <ipxact:name>gui_phase_shift_deg13</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg14" type="real">
          <ipxact:name>gui_phase_shift_deg14</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg15" type="real">
          <ipxact:name>gui_phase_shift_deg15</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg16" type="real">
          <ipxact:name>gui_phase_shift_deg16</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_phase_shift_deg17" type="real">
          <ipxact:name>gui_phase_shift_deg17</ipxact:name>
          <ipxact:displayName>Desired Phase Shift</ipxact:displayName>
          <ipxact:value>0.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle0" type="real">
          <ipxact:name>gui_duty_cycle0</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle1" type="real">
          <ipxact:name>gui_duty_cycle1</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle2" type="real">
          <ipxact:name>gui_duty_cycle2</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle3" type="real">
          <ipxact:name>gui_duty_cycle3</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle4" type="real">
          <ipxact:name>gui_duty_cycle4</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle5" type="real">
          <ipxact:name>gui_duty_cycle5</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle6" type="real">
          <ipxact:name>gui_duty_cycle6</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle7" type="real">
          <ipxact:name>gui_duty_cycle7</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle8" type="real">
          <ipxact:name>gui_duty_cycle8</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle9" type="real">
          <ipxact:name>gui_duty_cycle9</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle10" type="real">
          <ipxact:name>gui_duty_cycle10</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle11" type="real">
          <ipxact:name>gui_duty_cycle11</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle12" type="real">
          <ipxact:name>gui_duty_cycle12</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle13" type="real">
          <ipxact:name>gui_duty_cycle13</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle14" type="real">
          <ipxact:name>gui_duty_cycle14</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle15" type="real">
          <ipxact:name>gui_duty_cycle15</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle16" type="real">
          <ipxact:name>gui_duty_cycle16</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_duty_cycle17" type="real">
          <ipxact:name>gui_duty_cycle17</ipxact:name>
          <ipxact:displayName>Desired Duty Cycle</ipxact:displayName>
          <ipxact:value>50.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="gui_simulation_type" type="bit">
          <ipxact:name>gui_simulation_type</ipxact:name>
          <ipxact:displayName>Force full PLL simulation model</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hp_qsys_scripting_mode" type="bit">
          <ipxact:name>hp_qsys_scripting_mode</ipxact:name>
          <ipxact:displayName>hp_qsys_scripting_mode</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_module_parameters>
    <altera:altera_assignments>
      <ipxact:parameters>
        <ipxact:parameter parameterId="embeddedsw.dts.compatible" type="string">
          <ipxact:name>embeddedsw.dts.compatible</ipxact:name>
          <ipxact:value>altr,pll</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="embeddedsw.dts.group" type="string">
          <ipxact:name>embeddedsw.dts.group</ipxact:name>
          <ipxact:value>clock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="embeddedsw.dts.vendor" type="string">
          <ipxact:name>embeddedsw.dts.vendor</ipxact:name>
          <ipxact:value>altr</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_assignments>
    <altera:altera_system_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="board" type="string">
          <ipxact:name>board</ipxact:name>
          <ipxact:displayName>Board</ipxact:displayName>
          <ipxact:value>default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>Device</ipxact:displayName>
          <ipxact:value>A5EB013BB23BE4SCS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceFamily" type="string">
          <ipxact:name>deviceFamily</ipxact:name>
          <ipxact:displayName>Device family</ipxact:displayName>
          <ipxact:value>Agilex 5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceSpeedGrade" type="string">
          <ipxact:name>deviceSpeedGrade</ipxact:name>
          <ipxact:displayName>Device Speed Grade</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generationId" type="int">
          <ipxact:name>generationId</ipxact:name>
          <ipxact:displayName>Generation Id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bonusData" type="string">
          <ipxact:name>bonusData</ipxact:name>
          <ipxact:displayName>bonusData</ipxact:displayName>
          <ipxact:value>bonusData 
{
   element iopll_0
   {
      datum _sortIndex
      {
         value = "0";
         type = "int";
      }
   }
}
</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hideFromIPCatalog" type="bit">
          <ipxact:name>hideFromIPCatalog</ipxact:name>
          <ipxact:displayName>Hide from IP Catalog</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="lockedInterfaceDefinition" type="string">
          <ipxact:name>lockedInterfaceDefinition</ipxact:name>
          <ipxact:displayName>lockedInterfaceDefinition</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="systemInfos" type="string">
          <ipxact:name>systemInfos</ipxact:name>
          <ipxact:displayName>systemInfos</ipxact:displayName>
          <ipxact:value>&lt;systemInfosDefinition&gt;
    &lt;connPtSystemInfos&gt;
        &lt;entry&gt;
            &lt;key&gt;outclk0&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;outclk0&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;CLOCK_RATE&lt;/key&gt;
                        &lt;value&gt;12288136&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
    &lt;/connPtSystemInfos&gt;
&lt;/systemInfosDefinition&gt;</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dflBitArray" type="string">
          <ipxact:name>dflBitArray</ipxact:name>
          <ipxact:displayName>dflBitArray</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cpuInfo" type="string">
          <ipxact:name>cpuInfo</ipxact:name>
          <ipxact:displayName>cpuInfo</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_system_parameters>
    <altera:altera_interface_boundary>
      <altera:interface_mapping altera:name="locked" altera:internal="iopll_0.locked" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="locked" altera:internal="locked"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="outclk0" altera:internal="iopll_0.outclk0" altera:type="clock" altera:dir="start">
        <altera:port_mapping altera:name="outclk_0" altera:internal="outclk_0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="outclk1" altera:internal="iopll_0.outclk1"></altera:interface_mapping>
      <altera:interface_mapping altera:name="refclk" altera:internal="iopll_0.refclk" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="refclk" altera:internal="refclk"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="reset" altera:internal="iopll_0.reset" altera:type="reset" altera:dir="end">
        <altera:port_mapping altera:name="rst" altera:internal="rst"></altera:port_mapping>
      </altera:interface_mapping>
    </altera:altera_interface_boundary>
    <altera:altera_has_warnings>true</altera:altera_has_warnings>
    <altera:altera_has_errors>false</altera:altera_has_errors>
  </ipxact:vendorExtensions>
</ipxact:component>