<?xml version="1.0" ?>
<!--Your use of Altera Corporation's design tools, logic functions 
and other software and tools, and any partner logic 
functions, and any output files from any of the foregoing 
(including device programming or simulation files), and any 
associated documentation or information are expressly subject 
to the terms and conditions of the Altera Program License 
Subscription Agreement, the Altera Quartus Prime License Agreement,
the Altera FPGA IP License Agreement, or other applicable license
agreement, including, without limitation, that your use is for
the sole purpose of programming logic devices manufactured by
Altera and sold by Altera or its authorized distributors.-->
<ipxact:component xmlns:altera="http://www.altera.com/XMLSchema/IPXact2014/extensions" xmlns:ipxact="http://www.accellera.org/XMLSchema/IPXACT/1685-2014">
  <ipxact:vendor>Altera Corporation</ipxact:vendor>
  <ipxact:library>EMIF_Qsys_emif_ddr4a_0</ipxact:library>
  <ipxact:name>EMIF_Qsys_emif_ddr4a_0</ipxact:name>
  <ipxact:version>4.2.0</ipxact:version>
  <ipxact:busInterfaces>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4_clock_in</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="clock" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="clock" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_clock_in</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>core_init_n</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="reset" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="reset" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset_n</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>core_init_n</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4_ctrl_ready</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="reset" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="reset" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset_n</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_reset_n</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:master></ipxact:master>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedDirectReset" type="string">
          <ipxact:name>associatedDirectReset</ipxact:name>
          <ipxact:displayName>Associated direct reset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedResetSinks" type="string">
          <ipxact:name>associatedResetSinks</ipxact:name>
          <ipxact:displayName>Associated reset sinks</ipxact:displayName>
          <ipxact:value>none</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>NONE</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="axi4" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="axi4" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awaddr</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awaddr</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awburst</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awburst</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awlen</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awlen</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awlock</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awlock</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awqos</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awqos</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awsize</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awsize</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awuser</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awuser</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awprot</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awprot</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_awready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>araddr</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_araddr</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arburst</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arburst</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arlen</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arlen</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arlock</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arlock</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arqos</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arqos</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arsize</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arsize</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>aruser</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_aruser</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arprot</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arprot</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_arready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_wdata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wstrb</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_wstrb</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wlast</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_wlast</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_wvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_wready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_bready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_bid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bresp</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_bresp</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_bvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rdata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rlast</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rlast</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rresp</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rresp</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4_rvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>s0_axi4_clock_in</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>s0_axi4_ctrl_ready</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="optionalAssociatedReset" type="bit">
          <ipxact:name>optionalAssociatedReset</ipxact:name>
          <ipxact:displayName>Optional associated reset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="trustzoneAware" type="bit">
          <ipxact:name>trustzoneAware</ipxact:name>
          <ipxact:displayName>TrustZone-aware</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wakeupSignals" type="bit">
          <ipxact:name>wakeupSignals</ipxact:name>
          <ipxact:displayName>wakeupSignals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="uniqueIdSupport" type="bit">
          <ipxact:name>uniqueIdSupport</ipxact:name>
          <ipxact:displayName>uniqueIdSupport</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="poison" type="bit">
          <ipxact:name>poison</ipxact:name>
          <ipxact:displayName>poison</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="traceSignals" type="bit">
          <ipxact:name>traceSignals</ipxact:name>
          <ipxact:displayName>traceSignals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isTranslator" type="bit">
          <ipxact:name>isTranslator</ipxact:name>
          <ipxact:displayName>isTranslator</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingReads" type="longint">
          <ipxact:name>maximumOutstandingReads</ipxact:name>
          <ipxact:displayName>maximumOutstandingReads</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingWrites" type="longint">
          <ipxact:name>maximumOutstandingWrites</ipxact:name>
          <ipxact:displayName>maximumOutstandingWrites</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingTransactions" type="longint">
          <ipxact:name>maximumOutstandingTransactions</ipxact:name>
          <ipxact:displayName>maximumOutstandingTransactions</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dataCheck" type="bit">
          <ipxact:name>dataCheck</ipxact:name>
          <ipxact:displayName>dataCheck</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressCheck" type="bit">
          <ipxact:name>addressCheck</ipxact:name>
          <ipxact:displayName>addressCheck</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="securityAttribute" type="bit">
          <ipxact:name>securityAttribute</ipxact:name>
          <ipxact:displayName>securityAttribute</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="userData" type="bit">
          <ipxact:name>userData</ipxact:name>
          <ipxact:displayName>userData</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readAcceptanceCapability" type="longint">
          <ipxact:name>readAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Read acceptance capability</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeAcceptanceCapability" type="longint">
          <ipxact:name>writeAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Write acceptance capability</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="combinedAcceptanceCapability" type="longint">
          <ipxact:name>combinedAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Combined acceptance capability</ipxact:displayName>
          <ipxact:value>64</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readDataReorderingDepth" type="longint">
          <ipxact:name>readDataReorderingDepth</ipxact:name>
          <ipxact:displayName>Read data reordering depth</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToMaster" type="string">
          <ipxact:name>bridgesToMaster</ipxact:name>
          <ipxact:displayName>bridgesToMaster</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureGuid" type="string">
          <ipxact:name>dfhFeatureGuid</ipxact:name>
          <ipxact:displayName>Feature GUID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhGroupId" type="longint">
          <ipxact:name>dfhGroupId</ipxact:name>
          <ipxact:displayName>Group ID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterId" type="string">
          <ipxact:name>dfhParameterId</ipxact:name>
          <ipxact:displayName>ID</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterName" type="string">
          <ipxact:name>dfhParameterName</ipxact:name>
          <ipxact:displayName>Name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterVersion" type="string">
          <ipxact:name>dfhParameterVersion</ipxact:name>
          <ipxact:displayName>Version</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterData" type="string">
          <ipxact:name>dfhParameterData</ipxact:name>
          <ipxact:displayName>Data (HEX/DEC)</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterDataLength" type="string">
          <ipxact:name>dfhParameterDataLength</ipxact:name>
          <ipxact:displayName>Data length</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureMajorVersion" type="longint">
          <ipxact:name>dfhFeatureMajorVersion</ipxact:name>
          <ipxact:displayName>Feature major version</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureMinorVersion" type="longint">
          <ipxact:name>dfhFeatureMinorVersion</ipxact:name>
          <ipxact:displayName>Feature minor version</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureId" type="longint">
          <ipxact:name>dfhFeatureId</ipxact:name>
          <ipxact:displayName>Feature ID</ipxact:displayName>
          <ipxact:value>35</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureType" type="longint">
          <ipxact:name>dfhFeatureType</ipxact:name>
          <ipxact:displayName>Feature Type</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="noNarrowTransfer" type="bit">
          <ipxact:name>noNarrowTransfer</ipxact:name>
          <ipxact:displayName>noNarrowTransfer</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
      <ipxact:vendorExtensions>
        <altera:altera_assignments>
          <ipxact:parameters>
            <ipxact:parameter parameterId="mem_capacity_gbits" type="string">
              <ipxact:name>mem_capacity_gbits</ipxact:name>
              <ipxact:value>8.0</ipxact:value>
            </ipxact:parameter>
          </ipxact:parameters>
        </altera:altera_assignments>
      </ipxact:vendorExtensions>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4lite_clock</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="clock" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="clock" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_clock</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4lite_reset_n</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="reset" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="reset" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>reset_n</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_reset_n</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>s0_axi4lite_clock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="synchronousEdges" type="string">
          <ipxact:name>synchronousEdges</ipxact:name>
          <ipxact:displayName>Synchronous edges</ipxact:displayName>
          <ipxact:value>DEASSERT</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>s0_axi4lite</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="axi4lite" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="axi4lite" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awaddr</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_awaddr</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awprot</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_awprot</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_awvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>awready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_awready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>araddr</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_araddr</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arprot</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_arprot</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_arvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>arready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_arready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_wdata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wstrb</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_wstrb</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_wvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>wready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_wready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_bready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bresp</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_bresp</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>bvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_bvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rready</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_rready</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rdata</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_rdata</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rresp</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_rresp</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>rvalid</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>s0_axi4lite_rvalid</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>Associated clock</ipxact:displayName>
          <ipxact:value>s0_axi4lite_clock</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>Associated reset</ipxact:displayName>
          <ipxact:value>s0_axi4lite_reset_n</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="optionalAssociatedReset" type="bit">
          <ipxact:name>optionalAssociatedReset</ipxact:name>
          <ipxact:displayName>Optional associated reset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="trustzoneAware" type="bit">
          <ipxact:name>trustzoneAware</ipxact:name>
          <ipxact:displayName>trustzoneAware</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="wakeupSignals" type="bit">
          <ipxact:name>wakeupSignals</ipxact:name>
          <ipxact:displayName>wakeupSignals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="uniqueIdSupport" type="bit">
          <ipxact:name>uniqueIdSupport</ipxact:name>
          <ipxact:displayName>uniqueIdSupport</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="poison" type="bit">
          <ipxact:name>poison</ipxact:name>
          <ipxact:displayName>poison</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="traceSignals" type="bit">
          <ipxact:name>traceSignals</ipxact:name>
          <ipxact:displayName>traceSignals</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="isTranslator" type="bit">
          <ipxact:name>isTranslator</ipxact:name>
          <ipxact:displayName>isTranslator</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingReads" type="longint">
          <ipxact:name>maximumOutstandingReads</ipxact:name>
          <ipxact:displayName>maximumOutstandingReads</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingWrites" type="longint">
          <ipxact:name>maximumOutstandingWrites</ipxact:name>
          <ipxact:displayName>maximumOutstandingWrites</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="maximumOutstandingTransactions" type="longint">
          <ipxact:name>maximumOutstandingTransactions</ipxact:name>
          <ipxact:displayName>maximumOutstandingTransactions</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dataCheck" type="bit">
          <ipxact:name>dataCheck</ipxact:name>
          <ipxact:displayName>dataCheck</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="addressCheck" type="bit">
          <ipxact:name>addressCheck</ipxact:name>
          <ipxact:displayName>addressCheck</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="securityAttribute" type="bit">
          <ipxact:name>securityAttribute</ipxact:name>
          <ipxact:displayName>securityAttribute</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="userData" type="bit">
          <ipxact:name>userData</ipxact:name>
          <ipxact:displayName>userData</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readAcceptanceCapability" type="longint">
          <ipxact:name>readAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Read acceptance capability</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="writeAcceptanceCapability" type="longint">
          <ipxact:name>writeAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Write acceptance capability</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="combinedAcceptanceCapability" type="longint">
          <ipxact:name>combinedAcceptanceCapability</ipxact:name>
          <ipxact:displayName>Combined acceptance capability</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="readDataReorderingDepth" type="longint">
          <ipxact:name>readDataReorderingDepth</ipxact:name>
          <ipxact:displayName>Read data reordering depth</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bridgesToMaster" type="string">
          <ipxact:name>bridgesToMaster</ipxact:name>
          <ipxact:displayName>bridgesToMaster</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureGuid" type="string">
          <ipxact:name>dfhFeatureGuid</ipxact:name>
          <ipxact:displayName>Feature GUID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhGroupId" type="longint">
          <ipxact:name>dfhGroupId</ipxact:name>
          <ipxact:displayName>Group ID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterId" type="string">
          <ipxact:name>dfhParameterId</ipxact:name>
          <ipxact:displayName>ID</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterName" type="string">
          <ipxact:name>dfhParameterName</ipxact:name>
          <ipxact:displayName>Name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterVersion" type="string">
          <ipxact:name>dfhParameterVersion</ipxact:name>
          <ipxact:displayName>Version</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterData" type="string">
          <ipxact:name>dfhParameterData</ipxact:name>
          <ipxact:displayName>Data (HEX/DEC)</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhParameterDataLength" type="string">
          <ipxact:name>dfhParameterDataLength</ipxact:name>
          <ipxact:displayName>Data length</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureMajorVersion" type="longint">
          <ipxact:name>dfhFeatureMajorVersion</ipxact:name>
          <ipxact:displayName>Feature major version</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureMinorVersion" type="longint">
          <ipxact:name>dfhFeatureMinorVersion</ipxact:name>
          <ipxact:displayName>Feature minor version</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureId" type="longint">
          <ipxact:name>dfhFeatureId</ipxact:name>
          <ipxact:displayName>Feature ID</ipxact:displayName>
          <ipxact:value>35</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dfhFeatureType" type="longint">
          <ipxact:name>dfhFeatureType</ipxact:name>
          <ipxact:displayName>Feature Type</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>mem_0</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_cs</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_cs</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_ca</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_ca</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_cke</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_cke</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_dq</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_dq</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_dqs_t</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_dqs_t</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_dqs_c</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_dqs_c</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_dmi</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_dmi</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>mem_ck_0</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_ck_t</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_ck_t</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_ck_c</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_ck_c</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>mem_reset_n</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>mem_reset_n</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>mem_0_reset_n</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>oct_0</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="conduit" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>oct_rzqin</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>oct_rzqin_0</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="associatedClock" type="string">
          <ipxact:name>associatedClock</ipxact:name>
          <ipxact:displayName>associatedClock</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="associatedReset" type="string">
          <ipxact:name>associatedReset</ipxact:name>
          <ipxact:displayName>associatedReset</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="prSafe" type="bit">
          <ipxact:name>prSafe</ipxact:name>
          <ipxact:displayName>Partial Reconfiguration Safe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
    <ipxact:busInterface>
      <ipxact:name>ref_clk</ipxact:name>
      <ipxact:busType vendor="intel" library="intel" name="clock" version="26.1"></ipxact:busType>
      <ipxact:abstractionTypes>
        <ipxact:abstractionType>
          <ipxact:abstractionRef vendor="intel" library="intel" name="clock" version="26.1"></ipxact:abstractionRef>
          <ipxact:portMaps>
            <ipxact:portMap>
              <ipxact:logicalPort>
                <ipxact:name>clk</ipxact:name>
              </ipxact:logicalPort>
              <ipxact:physicalPort>
                <ipxact:name>ref_clk</ipxact:name>
              </ipxact:physicalPort>
            </ipxact:portMap>
          </ipxact:portMaps>
        </ipxact:abstractionType>
      </ipxact:abstractionTypes>
      <ipxact:slave></ipxact:slave>
      <ipxact:parameters>
        <ipxact:parameter parameterId="clockRate" type="longint">
          <ipxact:name>clockRate</ipxact:name>
          <ipxact:displayName>Clock rate</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="externallyDriven" type="bit">
          <ipxact:name>externallyDriven</ipxact:name>
          <ipxact:displayName>Externally driven</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ptfSchematicName" type="string">
          <ipxact:name>ptfSchematicName</ipxact:name>
          <ipxact:displayName>PTF schematic name</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </ipxact:busInterface>
  </ipxact:busInterfaces>
  <ipxact:model>
    <ipxact:views>
      <ipxact:view>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:envIdentifier>:quartus.altera.com:</ipxact:envIdentifier>
        <ipxact:componentInstantiationRef>QUARTUS_SYNTH</ipxact:componentInstantiationRef>
      </ipxact:view>
    </ipxact:views>
    <ipxact:instantiations>
      <ipxact:componentInstantiation>
        <ipxact:name>QUARTUS_SYNTH</ipxact:name>
        <ipxact:moduleName>emif_io96b_lpddr4</ipxact:moduleName>
        <ipxact:fileSetRef>
          <ipxact:localName>QUARTUS_SYNTH</ipxact:localName>
        </ipxact:fileSetRef>
      </ipxact:componentInstantiation>
    </ipxact:instantiations>
    <ipxact:ports>
      <ipxact:port>
        <ipxact:name>s0_axi4_clock_in</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>core_init_n</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_reset_n</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awaddr</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>29</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awburst</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awlen</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awlock</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awqos</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awsize</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awuser</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>13</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awprot</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_awready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_araddr</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>29</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arburst</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arlen</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>7</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arlock</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arqos</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arsize</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_aruser</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>13</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arprot</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_arready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_wdata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>255</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_wstrb</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_wlast</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_wvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_wready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_bready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_bid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_bresp</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_bvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rdata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>255</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>6</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rlast</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rresp</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4_rvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_clock</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_reset_n</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_awaddr</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>26</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_awprot</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_awvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_awready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_araddr</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>26</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_arprot</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>2</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_arvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_arready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_wdata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_wstrb</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_wvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_wready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_bready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_bresp</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_bvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_rready</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_rdata</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_rresp</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>1</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>s0_axi4lite_rvalid</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_cs</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_ca</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>5</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_cke</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_dq</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>inout</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>31</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_dqs_t</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>inout</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_dqs_c</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>inout</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_dmi</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>inout</ipxact:direction>
          <ipxact:vectors>
            <ipxact:vector>
              <ipxact:left>0</ipxact:left>
              <ipxact:right>3</ipxact:right>
            </ipxact:vector>
          </ipxact:vectors>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_ck_t</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_ck_c</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC_VECTOR</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>mem_0_reset_n</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>out</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>oct_rzqin_0</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
      <ipxact:port>
        <ipxact:name>ref_clk</ipxact:name>
        <ipxact:wire>
          <ipxact:direction>in</ipxact:direction>
          <ipxact:wireTypeDefs>
            <ipxact:wireTypeDef>
              <ipxact:typeName>STD_LOGIC</ipxact:typeName>
              <ipxact:viewRef>QUARTUS_SYNTH</ipxact:viewRef>
            </ipxact:wireTypeDef>
          </ipxact:wireTypeDefs>
        </ipxact:wire>
      </ipxact:port>
    </ipxact:ports>
  </ipxact:model>
  <ipxact:vendorExtensions>
    <altera:entity_info>
      <ipxact:vendor>Altera Corporation</ipxact:vendor>
      <ipxact:library>EMIF_Qsys_emif_ddr4a_0</ipxact:library>
      <ipxact:name>emif_io96b_lpddr4</ipxact:name>
      <ipxact:version>4.2.0</ipxact:version>
    </altera:entity_info>
    <altera:altera_module_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="SYSINFO_BOARD" type="string">
          <ipxact:name>SYSINFO_BOARD</ipxact:name>
          <ipxact:displayName>SYSINFO_BOARD</ipxact:displayName>
          <ipxact:value>default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_BOARD_TRAIT" type="string">
          <ipxact:name>SYSINFO_BOARD_TRAIT</ipxact:name>
          <ipxact:displayName>SYSINFO_BOARD_TRAIT</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE" type="string">
          <ipxact:name>SYSINFO_DEVICE</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE</ipxact:displayName>
          <ipxact:value>A5EB013BB23BE4SCS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_FAMILY" type="string">
          <ipxact:name>SYSINFO_DEVICE_FAMILY</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_FAMILY</ipxact:displayName>
          <ipxact:value>Agilex 5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_SPEEDGRADE" type="string">
          <ipxact:name>SYSINFO_DEVICE_SPEEDGRADE</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_SPEEDGRADE</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_DIE_REVISIONS" type="string">
          <ipxact:name>SYSINFO_DEVICE_DIE_REVISIONS</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_DIE_REVISIONS</ipxact:displayName>
          <ipxact:value>MAIN_SM4_REVB</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_TEMPERATURE_GRADE" type="string">
          <ipxact:name>SYSINFO_DEVICE_TEMPERATURE_GRADE</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_TEMPERATURE_GRADE</ipxact:displayName>
          <ipxact:value>EXTENDED</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_POWER_MODEL" type="string">
          <ipxact:name>SYSINFO_DEVICE_POWER_MODEL</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_POWER_MODEL</ipxact:displayName>
          <ipxact:value>STANDARD_POWER_FIXED</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_SUPPORTS_VID" type="string">
          <ipxact:name>SYSINFO_SUPPORTS_VID</ipxact:name>
          <ipxact:displayName>SYSINFO_SUPPORTS_VID</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_IOBANK_REVISION" type="string">
          <ipxact:name>SYSINFO_DEVICE_IOBANK_REVISION</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_IOBANK_REVISION</ipxact:displayName>
          <ipxact:value>IO96B_REVB1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_GROUP" type="string">
          <ipxact:name>SYSINFO_DEVICE_GROUP</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_GROUP</ipxact:displayName>
          <ipxact:value>B</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="SYSINFO_DEVICE_BASE_DIE" type="string">
          <ipxact:name>SYSINFO_DEVICE_BASE_DIE</ipxact:name>
          <ipxact:displayName>SYSINFO_DEVICE_BASE_DIE</ipxact:displayName>
          <ipxact:value>SM4REVB</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TECH_IS_X" type="bit">
          <ipxact:name>MEM_TECH_IS_X</ipxact:name>
          <ipxact:displayName>Use LPDDR4X</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_NUM_CHANNELS" type="int">
          <ipxact:name>MEM_NUM_CHANNELS</ipxact:name>
          <ipxact:displayName>Number of Channels</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_CHANNEL_DATA_DQ_WIDTH" type="int">
          <ipxact:name>MEM_CHANNEL_DATA_DQ_WIDTH</ipxact:name>
          <ipxact:displayName>Data DQ Width</ipxact:displayName>
          <ipxact:value>32</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_DIE_DENSITY_GBITS" type="int">
          <ipxact:name>MEM_DIE_DENSITY_GBITS</ipxact:name>
          <ipxact:displayName>Die Density</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_CHANNEL_CS_WIDTH" type="string">
          <ipxact:name>MEM_CHANNEL_CS_WIDTH</ipxact:name>
          <ipxact:displayName>CS Width</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_OPERATING_FREQ_MHZ_AUTOSET_EN" type="bit">
          <ipxact:name>MEM_OPERATING_FREQ_MHZ_AUTOSET_EN</ipxact:name>
          <ipxact:displayName>Auto-set Memory Operating Frequency</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_OPERATING_FREQ_MHZ" type="string">
          <ipxact:name>MEM_OPERATING_FREQ_MHZ</ipxact:name>
          <ipxact:displayName>Memory Operating Frequency</ipxact:displayName>
          <ipxact:value>1066.667</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_ECC_INLINE_EN" type="bit">
          <ipxact:name>CTRL_ECC_INLINE_EN</ipxact:name>
          <ipxact:displayName>Use In-Line ECC</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_ECC_AUTOCORRECT_EN" type="bit">
          <ipxact:name>CTRL_ECC_AUTOCORRECT_EN</ipxact:name>
          <ipxact:displayName>Use ECC Autocorrection</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_DM_EN" type="bit">
          <ipxact:name>CTRL_DM_EN</ipxact:name>
          <ipxact:displayName>Use Data Masking</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_WR_DBI_EN" type="bit">
          <ipxact:name>CTRL_WR_DBI_EN</ipxact:name>
          <ipxact:displayName>Use WDBI</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_RD_DBI_EN" type="bit">
          <ipxact:name>CTRL_RD_DBI_EN</ipxact:name>
          <ipxact:displayName>Use RDBI</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_SCRAMBLER_EN" type="bit">
          <ipxact:name>CTRL_SCRAMBLER_EN</ipxact:name>
          <ipxact:displayName>CTRL_SCRAMBLER_EN</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_PERFORMANCE_PROFILE" type="string">
          <ipxact:name>CTRL_PERFORMANCE_PROFILE</ipxact:name>
          <ipxact:displayName>Controller Performance Profile</ipxact:displayName>
          <ipxact:value>SEQ</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_AUTO_PRECHARGE_EN" type="bit">
          <ipxact:name>CTRL_AUTO_PRECHARGE_EN</ipxact:name>
          <ipxact:displayName>Force Auto-Precharge</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="DIAG_HMC_ADDR_SWAP_EN" type="bit">
          <ipxact:name>DIAG_HMC_ADDR_SWAP_EN</ipxact:name>
          <ipxact:displayName>Enable Row/CS Swap</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_PLACEMENT_EN" type="bit">
          <ipxact:name>CTRL_PLACEMENT_EN</ipxact:name>
          <ipxact:displayName>Enable Placement Logic</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_ALL_STRB_EN" type="bit">
          <ipxact:name>CTRL_ALL_STRB_EN</ipxact:name>
          <ipxact:displayName>Enable All Strobe</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_FIXED_PRIORITY_EN" type="bit">
          <ipxact:name>CTRL_FIXED_PRIORITY_EN</ipxact:name>
          <ipxact:displayName>Enable Fixed Priority</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_FIXED_W_PRIORITY" type="int">
          <ipxact:name>CTRL_FIXED_W_PRIORITY</ipxact:name>
          <ipxact:displayName>Fixed Write Priority</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="CTRL_FIXED_R_PRIORITY" type="int">
          <ipxact:name>CTRL_FIXED_R_PRIORITY</ipxact:name>
          <ipxact:displayName>Fixed Read Priority</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_R2W_SAMECS_CYC" type="int">
          <ipxact:name>TURNAROUND_R2W_SAMECS_CYC</ipxact:name>
          <ipxact:displayName>Additional read-to-write turnaround time (same rank)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_R2R_SAMECS_CYC" type="int">
          <ipxact:name>TURNAROUND_R2R_SAMECS_CYC</ipxact:name>
          <ipxact:displayName>Additional read-to-read turnaround time (same rank)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_W2W_SAMECS_CYC" type="int">
          <ipxact:name>TURNAROUND_W2W_SAMECS_CYC</ipxact:name>
          <ipxact:displayName>Additional write-to-write turnaround time (same rank)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_W2R_SAMECS_CYC" type="int">
          <ipxact:name>TURNAROUND_W2R_SAMECS_CYC</ipxact:name>
          <ipxact:displayName>Additional write-to-read turnaround time (same rank)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_R2W_DIFFCS_CYC" type="int">
          <ipxact:name>TURNAROUND_R2W_DIFFCS_CYC</ipxact:name>
          <ipxact:displayName>Additional read-to-write turnaround time (different ranks)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_R2R_DIFFCS_CYC" type="int">
          <ipxact:name>TURNAROUND_R2R_DIFFCS_CYC</ipxact:name>
          <ipxact:displayName>Additional read-to-read turnaround time (different ranks)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_W2W_DIFFCS_CYC" type="int">
          <ipxact:name>TURNAROUND_W2W_DIFFCS_CYC</ipxact:name>
          <ipxact:displayName>Additional write-to-write turnaround time (different ranks)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="TURNAROUND_W2R_DIFFCS_CYC" type="int">
          <ipxact:name>TURNAROUND_W2R_DIFFCS_CYC</ipxact:name>
          <ipxact:displayName>Additional write-to-read turnaround time (different ranks)</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_REFCLK_FREQ_MHZ_AUTOSET_EN" type="bit">
          <ipxact:name>PHY_REFCLK_FREQ_MHZ_AUTOSET_EN</ipxact:name>
          <ipxact:displayName>Auto-set PLL Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_REFCLK_ADVANCED_SELECT_EN" type="bit">
          <ipxact:name>PHY_REFCLK_ADVANCED_SELECT_EN</ipxact:name>
          <ipxact:displayName>Enable Advanced List of PLL Reference Clock Frequencies</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_REFCLK_FREQ_MHZ" type="string">
          <ipxact:name>PHY_REFCLK_FREQ_MHZ</ipxact:name>
          <ipxact:displayName>Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>166.6667</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_AC_PLACEMENT" type="string">
          <ipxact:name>PHY_AC_PLACEMENT</ipxact:name>
          <ipxact:displayName>AC Placement</ipxact:displayName>
          <ipxact:value>BOT</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_MAINBAND_ACCESS_MODE_AUTOSET_EN" type="bit">
          <ipxact:name>PHY_MAINBAND_ACCESS_MODE_AUTOSET_EN</ipxact:name>
          <ipxact:displayName>Auto-set Mainband Access Mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_MAINBAND_ACCESS_MODE" type="string">
          <ipxact:name>PHY_MAINBAND_ACCESS_MODE</ipxact:name>
          <ipxact:displayName>Mainband Access Mode</ipxact:displayName>
          <ipxact:value>ASYNC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_SIDEBAND_ACCESS_MODE_AUTOSET_EN" type="bit">
          <ipxact:name>PHY_SIDEBAND_ACCESS_MODE_AUTOSET_EN</ipxact:name>
          <ipxact:displayName>Auto-set Sideband Access Mode</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_SIDEBAND_ACCESS_MODE" type="string">
          <ipxact:name>PHY_SIDEBAND_ACCESS_MODE</ipxact:name>
          <ipxact:displayName>Sideband Access Mode</ipxact:displayName>
          <ipxact:value>FABRIC</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_SWIZZLE_MAP" type="string">
          <ipxact:name>PHY_SWIZZLE_MAP</ipxact:name>
          <ipxact:displayName>Pin Swizzle Map</ipxact:displayName>
          <ipxact:value>PIN_SWIZZLE_CH0_DQS0=0,1,6,7,2,4,5,3;PIN_SWIZZLE_CH0_DQS1=15,14,8,9,13,12,10,11;PIN_SWIZZLE_CH0_DQS2=18,17,21,19,20,16,22,23;PIN_SWIZZLE_CH0_DQS3=26,28,27,29,25,24,31,30;</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="DEBUG_TOOLS_EN" type="bit">
          <ipxact:name>DEBUG_TOOLS_EN</ipxact:name>
          <ipxact:displayName>Use Debug Toolkit</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="DEBUG_PRINT_LEVEL" type="int">
          <ipxact:name>DEBUG_PRINT_LEVEL</ipxact:name>
          <ipxact:displayName>Debug Print Level</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="INSTANCE_ID" type="int">
          <ipxact:name>INSTANCE_ID</ipxact:name>
          <ipxact:displayName>Instance ID</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ADV_CAL_ENABLE_MARGIN" type="bit">
          <ipxact:name>ADV_CAL_ENABLE_MARGIN</ipxact:name>
          <ipxact:displayName>Enable Margining during Calibration</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ADV_CAL_ENABLE_REQ" type="bit">
          <ipxact:name>ADV_CAL_ENABLE_REQ</ipxact:name>
          <ipxact:displayName>Enable REQ Calibration</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ADV_CAL_ENABLE_WEQ" type="bit">
          <ipxact:name>ADV_CAL_ENABLE_WEQ</ipxact:name>
          <ipxact:displayName>Enable WEQ Calibration</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_WLS" type="real">
          <ipxact:name>MEM_WLS</ipxact:name>
          <ipxact:displayName>MEM_WLS</ipxact:displayName>
          <ipxact:value>1.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_CL_CYC" type="int">
          <ipxact:name>MEM_CL_CYC</ipxact:name>
          <ipxact:displayName>Read Latency</ipxact:displayName>
          <ipxact:value>22</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_CWL_CYC" type="int">
          <ipxact:name>MEM_CWL_CYC</ipxact:name>
          <ipxact:displayName>Write Latency</ipxact:displayName>
          <ipxact:value>18</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_PER_BANK_REF_EN" type="int">
          <ipxact:name>MEM_PER_BANK_REF_EN</ipxact:name>
          <ipxact:displayName>MEM_PER_BANK_REF_EN</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_RD_PREAMBLE_CYC" type="int">
          <ipxact:name>MEM_RD_PREAMBLE_CYC</ipxact:name>
          <ipxact:displayName>MEM_RD_PREAMBLE_CYC</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_RD_POSTAMBLE_CYC" type="int">
          <ipxact:name>MEM_RD_POSTAMBLE_CYC</ipxact:name>
          <ipxact:displayName>Read Postamble Cycles</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_WR_POSTAMBLE_CYC" type="int">
          <ipxact:name>MEM_WR_POSTAMBLE_CYC</ipxact:name>
          <ipxact:displayName>Write Postamble Cycles</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TSR_NS" type="real">
          <ipxact:name>MEM_TSR_NS</ipxact:name>
          <ipxact:displayName>tSR</ipxact:displayName>
          <ipxact:value>15.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRFCAB_NS" type="real">
          <ipxact:name>MEM_TRFCAB_NS</ipxact:name>
          <ipxact:displayName>tRFCab</ipxact:displayName>
          <ipxact:value>180.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRFCPB_NS" type="real">
          <ipxact:name>MEM_TRFCPB_NS</ipxact:name>
          <ipxact:displayName>tRFCpb</ipxact:displayName>
          <ipxact:value>90.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TXSR_NS" type="real">
          <ipxact:name>MEM_TXSR_NS</ipxact:name>
          <ipxact:displayName>tXSR</ipxact:displayName>
          <ipxact:value>187.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TXP_NS" type="real">
          <ipxact:name>MEM_TXP_NS</ipxact:name>
          <ipxact:displayName>tXP</ipxact:displayName>
          <ipxact:value>7.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCCD_NS" type="real">
          <ipxact:name>MEM_TCCD_NS</ipxact:name>
          <ipxact:displayName>tCCD</ipxact:displayName>
          <ipxact:value>16.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRTP_NS" type="real">
          <ipxact:name>MEM_TRTP_NS</ipxact:name>
          <ipxact:displayName>tRTP</ipxact:displayName>
          <ipxact:value>7.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRCD_NS" type="real">
          <ipxact:name>MEM_TRCD_NS</ipxact:name>
          <ipxact:displayName>tRCD</ipxact:displayName>
          <ipxact:value>18.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRPPB_NS" type="real">
          <ipxact:name>MEM_TRPPB_NS</ipxact:name>
          <ipxact:displayName>tRPpb</ipxact:displayName>
          <ipxact:value>18.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRPAB_NS" type="real">
          <ipxact:name>MEM_TRPAB_NS</ipxact:name>
          <ipxact:displayName>tRPab</ipxact:displayName>
          <ipxact:value>21.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRAS_NS" type="real">
          <ipxact:name>MEM_TRAS_NS</ipxact:name>
          <ipxact:displayName>tRAS</ipxact:displayName>
          <ipxact:value>42.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TWR_NS" type="real">
          <ipxact:name>MEM_TWR_NS</ipxact:name>
          <ipxact:displayName>tWR</ipxact:displayName>
          <ipxact:value>18.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TWTR_NS" type="real">
          <ipxact:name>MEM_TWTR_NS</ipxact:name>
          <ipxact:displayName>tWTR</ipxact:displayName>
          <ipxact:value>10.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRRD_NS" type="real">
          <ipxact:name>MEM_TRRD_NS</ipxact:name>
          <ipxact:displayName>tRRD</ipxact:displayName>
          <ipxact:value>10.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TPPD_CYC" type="real">
          <ipxact:name>MEM_TPPD_CYC</ipxact:name>
          <ipxact:displayName>MEM_TPPD_CYC</ipxact:displayName>
          <ipxact:value>4.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TFAW_NS" type="real">
          <ipxact:name>MEM_TFAW_NS</ipxact:name>
          <ipxact:displayName>tFAW</ipxact:displayName>
          <ipxact:value>40.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TRC_NS" type="real">
          <ipxact:name>MEM_TRC_NS</ipxact:name>
          <ipxact:displayName>tRC</ipxact:displayName>
          <ipxact:value>63.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TREFW_NS" type="real">
          <ipxact:name>MEM_TREFW_NS</ipxact:name>
          <ipxact:displayName>tREFW</ipxact:displayName>
          <ipxact:value>3.2E7</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_MINNUMREFSREQ" type="real">
          <ipxact:name>MEM_MINNUMREFSREQ</ipxact:name>
          <ipxact:displayName>Min Number of Refs Reqd</ipxact:displayName>
          <ipxact:value>8192.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TREFI_NS" type="real">
          <ipxact:name>MEM_TREFI_NS</ipxact:name>
          <ipxact:displayName>tREFI</ipxact:displayName>
          <ipxact:value>3904.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKE_NS" type="real">
          <ipxact:name>MEM_TCKE_NS</ipxact:name>
          <ipxact:displayName>tCKE</ipxact:displayName>
          <ipxact:value>7.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCMDCKE_NS" type="real">
          <ipxact:name>MEM_TCMDCKE_NS</ipxact:name>
          <ipxact:displayName>tCMDCKE</ipxact:displayName>
          <ipxact:value>2.81</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKELCK_NS" type="real">
          <ipxact:name>MEM_TCKELCK_NS</ipxact:name>
          <ipxact:displayName>tCKELCK</ipxact:displayName>
          <ipxact:value>5.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCSCKE_NS" type="real">
          <ipxact:name>MEM_TCSCKE_NS</ipxact:name>
          <ipxact:displayName>tCSCKE</ipxact:displayName>
          <ipxact:value>1.75</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKCKEH_NS" type="real">
          <ipxact:name>MEM_TCKCKEH_NS</ipxact:name>
          <ipxact:displayName>tCKCKEH</ipxact:displayName>
          <ipxact:value>2.81</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCSCKEH_NS" type="real">
          <ipxact:name>MEM_TCSCKEH_NS</ipxact:name>
          <ipxact:displayName>tCSCKEH</ipxact:displayName>
          <ipxact:value>1.75</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TMRWCKEL_NS" type="real">
          <ipxact:name>MEM_TMRWCKEL_NS</ipxact:name>
          <ipxact:displayName>tMRWCKEL</ipxact:displayName>
          <ipxact:value>14.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TZQCKE_NS" type="real">
          <ipxact:name>MEM_TZQCKE_NS</ipxact:name>
          <ipxact:displayName>tZQCKE</ipxact:displayName>
          <ipxact:value>2.81</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TMRR_NS" type="real">
          <ipxact:name>MEM_TMRR_NS</ipxact:name>
          <ipxact:displayName>tMRR</ipxact:displayName>
          <ipxact:value>7.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TMRW_NS" type="real">
          <ipxact:name>MEM_TMRW_NS</ipxact:name>
          <ipxact:displayName>tMRW</ipxact:displayName>
          <ipxact:value>10.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TMRD_NS" type="real">
          <ipxact:name>MEM_TMRD_NS</ipxact:name>
          <ipxact:displayName>tMRD</ipxact:displayName>
          <ipxact:value>14.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TESCKE_NS" type="real">
          <ipxact:name>MEM_TESCKE_NS</ipxact:name>
          <ipxact:displayName>tESCKE</ipxact:displayName>
          <ipxact:value>2.81</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TZQCAL_NS" type="real">
          <ipxact:name>MEM_TZQCAL_NS</ipxact:name>
          <ipxact:displayName>tZQCAL</ipxact:displayName>
          <ipxact:value>1000.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TZQLAT_NS" type="real">
          <ipxact:name>MEM_TZQLAT_NS</ipxact:name>
          <ipxact:displayName>tZQLAT</ipxact:displayName>
          <ipxact:value>30.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TDQSCK_MAX_NS" type="real">
          <ipxact:name>MEM_TDQSCK_MAX_NS</ipxact:name>
          <ipxact:displayName>tDQSCK_MAX</ipxact:displayName>
          <ipxact:value>3.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TDQSCK_MIN_NS" type="real">
          <ipxact:name>MEM_TDQSCK_MIN_NS</ipxact:name>
          <ipxact:displayName>tDQSCK_MIN</ipxact:displayName>
          <ipxact:value>1.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKCKEL_NS" type="real">
          <ipxact:name>MEM_TCKCKEL_NS</ipxact:name>
          <ipxact:displayName>tCKCKEL</ipxact:displayName>
          <ipxact:value>5.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKELCMD_NS" type="real">
          <ipxact:name>MEM_TCKELCMD_NS</ipxact:name>
          <ipxact:displayName>tCKELCMD</ipxact:displayName>
          <ipxact:value>5.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_TCKEHCMD_NS" type="real">
          <ipxact:name>MEM_TCKEHCMD_NS</ipxact:name>
          <ipxact:displayName>tCKEHCMD</ipxact:displayName>
          <ipxact:value>7.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="JEDEC_OVERRIDE_TABLE_PARAM_NAME" type="string">
          <ipxact:name>JEDEC_OVERRIDE_TABLE_PARAM_NAME</ipxact:name>
          <ipxact:displayName>JEDEC Parameter</ipxact:displayName>
          <ipxact:value>MEM_TRFCPB_NS,MEM_TCCD_NS,MEM_TCMDCKE_NS,MEM_TCKCKEH_NS,MEM_TZQCKE_NS,MEM_TESCKE_NS,MEM_RD_POSTAMBLE_CYC,MEM_WR_POSTAMBLE_CYC,MEM_TRFCAB_NS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="DIAG_EXTRA_PARAMETERS" type="string">
          <ipxact:name>DIAG_EXTRA_PARAMETERS</ipxact:name>
          <ipxact:displayName>Extra Diagnostic Parameters</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="DIAG_FORCE_SLIM_EN" type="bit">
          <ipxact:name>DIAG_FORCE_SLIM_EN</ipxact:name>
          <ipxact:displayName>DIAG_FORCE_SLIM_EN</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="IS_HPS" type="bit">
          <ipxact:name>IS_HPS</ipxact:name>
          <ipxact:displayName>IS_HPS</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EMIF_INST_NAME" type="string">
          <ipxact:name>EMIF_INST_NAME</ipxact:name>
          <ipxact:displayName>EMIF_INST_NAME</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_HDL_FORMAT" type="string">
          <ipxact:name>EX_DESIGN_HDL_FORMAT</ipxact:name>
          <ipxact:displayName>HDL Selection</ipxact:displayName>
          <ipxact:value>VERILOG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_GEN_SYNTH" type="bit">
          <ipxact:name>EX_DESIGN_GEN_SYNTH</ipxact:name>
          <ipxact:displayName>Generate Synthesis Fileset</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_GEN_SIM" type="bit">
          <ipxact:name>EX_DESIGN_GEN_SIM</ipxact:name>
          <ipxact:displayName>Generate Simulation Fileset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_GEN_CDC" type="bit">
          <ipxact:name>EX_DESIGN_GEN_CDC</ipxact:name>
          <ipxact:displayName>Generate CDC Fileset</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_TG_CSR_ACCESS_MODE" type="string">
          <ipxact:name>EX_DESIGN_TG_CSR_ACCESS_MODE</ipxact:name>
          <ipxact:displayName>Traffic Generator Remote Access</ipxact:displayName>
          <ipxact:value>JTAG</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_TG_PROGRAM" type="string">
          <ipxact:name>EX_DESIGN_TG_PROGRAM</ipxact:name>
          <ipxact:displayName>Traffic Generator Program</ipxact:displayName>
          <ipxact:value>MEDIUM</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_TG_WIDE_IF" type="bit">
          <ipxact:name>EX_DESIGN_TG_WIDE_IF</ipxact:name>
          <ipxact:displayName>Use 512-bit Traffic Generator</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ_AUTOSET_EN" type="bit">
          <ipxact:name>EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ_AUTOSET_EN</ipxact:name>
          <ipxact:displayName>Auto-set User PLL Output Clock Frequency</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ" type="real">
          <ipxact:name>EX_DESIGN_USER_PLL_OUTPUT_FREQ_MHZ</ipxact:name>
          <ipxact:displayName>User PLL Output Clock Frequency</ipxact:displayName>
          <ipxact:value>275.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_USER_PLL_REFCLK_FREQ_MHZ" type="real">
          <ipxact:name>EX_DESIGN_USER_PLL_REFCLK_FREQ_MHZ</ipxact:name>
          <ipxact:displayName>User PLL Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>100.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_NOC_PLL_REFCLK_FREQ_MHZ" type="int">
          <ipxact:name>EX_DESIGN_NOC_PLL_REFCLK_FREQ_MHZ</ipxact:name>
          <ipxact:displayName>NOC Reference Clock Frequency</ipxact:displayName>
          <ipxact:value>100</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_PMON_CH0_EN" type="bit">
          <ipxact:name>EX_DESIGN_PMON_CH0_EN</ipxact:name>
          <ipxact:displayName>Enable Performance Monitor for Channel 0</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_PMON_CH1_EN" type="bit">
          <ipxact:name>EX_DESIGN_PMON_CH1_EN</ipxact:name>
          <ipxact:displayName>Enable Performance Monitor for Channel 1</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_PMON_CH2_EN" type="bit">
          <ipxact:name>EX_DESIGN_PMON_CH2_EN</ipxact:name>
          <ipxact:displayName>Enable Performance Monitor for Channel 2</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_PMON_CH3_EN" type="bit">
          <ipxact:name>EX_DESIGN_PMON_CH3_EN</ipxact:name>
          <ipxact:displayName>Enable Performance Monitor for Channel 3</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="EX_DESIGN_PMON_INTERNAL_JAMB_EN" type="bit">
          <ipxact:name>EX_DESIGN_PMON_INTERNAL_JAMB_EN</ipxact:name>
          <ipxact:displayName>EX_DESIGN_PMON_INTERNAL_JAMB_EN</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_S_AC_OUTPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_S_AC_OUTPUT_OHM</ipxact:name>
          <ipxact:displayName>Phy AC Drive Strength</ipxact:displayName>
          <ipxact:value>SERIES_40_OHM_CAL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_S_CS_OUTPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_S_CS_OUTPUT_OHM</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_R_S_CS_OUTPUT_OHM</ipxact:displayName>
          <ipxact:value>SERIES_40_OHM_CAL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_S_CK_OUTPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_S_CK_OUTPUT_OHM</ipxact:name>
          <ipxact:displayName>Phy CK Drive Strength</ipxact:displayName>
          <ipxact:value>SERIES_40_OHM_CAL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_DQ_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_DQ_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_DQ_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>LVSTL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_S_DQ_OUTPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_S_DQ_OUTPUT_OHM</ipxact:name>
          <ipxact:displayName>Phy DQ Drive Strength</ipxact:displayName>
          <ipxact:value>SERIES_40_OHM_CAL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_DQ_SLEW_RATE" type="string">
          <ipxact:name>PHY_TERM_X_DQ_SLEW_RATE</ipxact:name>
          <ipxact:displayName>Phy DQ Slew Rate</ipxact:displayName>
          <ipxact:value>FASTEST</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_AC_SLEW_RATE" type="string">
          <ipxact:name>PHY_TERM_X_AC_SLEW_RATE</ipxact:name>
          <ipxact:displayName>Phy AC Slew Rate</ipxact:displayName>
          <ipxact:value>FASTEST</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_CS_SLEW_RATE" type="string">
          <ipxact:name>PHY_TERM_X_CS_SLEW_RATE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_CS_SLEW_RATE</ipxact:displayName>
          <ipxact:value>FASTEST</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_CK_SLEW_RATE" type="string">
          <ipxact:name>PHY_TERM_X_CK_SLEW_RATE</ipxact:name>
          <ipxact:displayName>Phy CK Slew Rate</ipxact:displayName>
          <ipxact:value>FASTEST</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_T_DQ_INPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_T_DQ_INPUT_OHM</ipxact:name>
          <ipxact:displayName>Phy DQ Input Termination</ipxact:displayName>
          <ipxact:value>RT_50_OHM_CAL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_DQ_VREF" type="real">
          <ipxact:name>PHY_TERM_X_DQ_VREF</ipxact:name>
          <ipxact:displayName>Phy DQ Initial Vrefin</ipxact:displayName>
          <ipxact:value>17.5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_DQS_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_DQS_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_DQS_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>DF_LVSTL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_T_REFCLK_INPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_T_REFCLK_INPUT_OHM</ipxact:name>
          <ipxact:displayName>Phy PLL Reference Clock Input Termination</ipxact:displayName>
          <ipxact:value>RT_DIFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_AC_OUTPUT_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_AC_OUTPUT_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_AC_OUTPUT_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>LVSTL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_CK_OUTPUT_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_CK_OUTPUT_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_CK_OUTPUT_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>DF_LVSTL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_CS_OUTPUT_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_CS_OUTPUT_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_CS_OUTPUT_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>LVSTL</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_GPIO_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_GPIO_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_GPIO_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>LVCMOS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_R_T_GPIO_INPUT_OHM" type="string">
          <ipxact:name>PHY_TERM_X_R_T_GPIO_INPUT_OHM</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_R_T_GPIO_INPUT_OHM</ipxact:displayName>
          <ipxact:value>RT_OFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_TERM_X_REFCLK_IO_STD_TYPE" type="string">
          <ipxact:name>PHY_TERM_X_REFCLK_IO_STD_TYPE</ipxact:name>
          <ipxact:displayName>PHY_TERM_X_REFCLK_IO_STD_TYPE</ipxact:displayName>
          <ipxact:value>TRUE_DIFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_AC_TX_EQUALIZATION" type="string">
          <ipxact:name>PHY_AC_TX_EQUALIZATION</ipxact:name>
          <ipxact:displayName>Phy AC TX Equalization (Deemphasis)</ipxact:displayName>
          <ipxact:value>OFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_CS_TX_EQUALIZATION" type="string">
          <ipxact:name>PHY_CS_TX_EQUALIZATION</ipxact:name>
          <ipxact:displayName>PHY_CS_TX_EQUALIZATION</ipxact:displayName>
          <ipxact:value>OFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_CK_TX_EQUALIZATION" type="string">
          <ipxact:name>PHY_CK_TX_EQUALIZATION</ipxact:name>
          <ipxact:displayName>Phy CK TX Equalization (Deemphasis)</ipxact:displayName>
          <ipxact:value>OFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="PHY_DQ_TX_EQUALIZATION" type="string">
          <ipxact:name>PHY_DQ_TX_EQUALIZATION</ipxact:name>
          <ipxact:displayName>Phy DQ TX Equalization (Deemphasis)</ipxact:displayName>
          <ipxact:value>OFF</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_DQ_X_TGT_WR" type="string">
          <ipxact:name>MEM_ODT_DQ_X_TGT_WR</ipxact:name>
          <ipxact:displayName>Mem Target Write Termination</ipxact:displayName>
          <ipxact:value>5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_DQ_X_IDLE" type="string">
          <ipxact:name>MEM_ODT_DQ_X_IDLE</ipxact:name>
          <ipxact:displayName>Mem DQ Idle Termination</ipxact:displayName>
          <ipxact:value>off</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_DQ_X_RON" type="string">
          <ipxact:name>MEM_ODT_DQ_X_RON</ipxact:name>
          <ipxact:displayName>Mem DQ Drive Strength</ipxact:displayName>
          <ipxact:value>6</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_VREF_DQ_X_RANGE" type="int">
          <ipxact:name>MEM_VREF_DQ_X_RANGE</ipxact:name>
          <ipxact:displayName>Mem VrefDQ Range</ipxact:displayName>
          <ipxact:value>1</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_VREF_DQ_X_VALUE" type="real">
          <ipxact:name>MEM_VREF_DQ_X_VALUE</ipxact:name>
          <ipxact:displayName>Mem VrefDQ Value</ipxact:displayName>
          <ipxact:value>18.0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_CA_X_CA_COMM" type="string">
          <ipxact:name>MEM_ODT_CA_X_CA_COMM</ipxact:name>
          <ipxact:displayName>Mem CA Common Termination</ipxact:displayName>
          <ipxact:value>3</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_CA_X_CA_ENABLE" type="string">
          <ipxact:name>MEM_ODT_CA_X_CA_ENABLE</ipxact:name>
          <ipxact:displayName>Mem CA Termination Enable</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_CA_X_CS_ENABLE" type="string">
          <ipxact:name>MEM_ODT_CA_X_CS_ENABLE</ipxact:name>
          <ipxact:displayName>Mem CS Termination Enable</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_ODT_CA_X_CK_ENABLE" type="string">
          <ipxact:name>MEM_ODT_CA_X_CK_ENABLE</ipxact:name>
          <ipxact:displayName>Mem CK Termination Enable</ipxact:displayName>
          <ipxact:value>true</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_VREF_CA_X_CA_RANGE" type="int">
          <ipxact:name>MEM_VREF_CA_X_CA_RANGE</ipxact:name>
          <ipxact:displayName>Mem VrefCA Range</ipxact:displayName>
          <ipxact:value>2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_VREF_CA_X_CA_VALUE" type="real">
          <ipxact:name>MEM_VREF_CA_X_CA_VALUE</ipxact:name>
          <ipxact:displayName>Mem VrefCA Value</ipxact:displayName>
          <ipxact:value>27.2</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_DQ_VREF" type="string">
          <ipxact:name>MEM_DQ_VREF</ipxact:name>
          <ipxact:displayName>MEM_DQ_VREF</ipxact:displayName>
          <ipxact:value>20</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="MEM_CA_VREF" type="string">
          <ipxact:name>MEM_CA_VREF</ipxact:name>
          <ipxact:displayName>MEM_CA_VREF</ipxact:displayName>
          <ipxact:value>13</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="ANALOG_PARAM_DERIVATION_PARAM_NAME" type="string">
          <ipxact:name>ANALOG_PARAM_DERIVATION_PARAM_NAME</ipxact:name>
          <ipxact:displayName>Analog Parameter</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_module_parameters>
    <altera:altera_system_parameters>
      <ipxact:parameters>
        <ipxact:parameter parameterId="board" type="string">
          <ipxact:name>board</ipxact:name>
          <ipxact:displayName>Board</ipxact:displayName>
          <ipxact:value>default</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="device" type="string">
          <ipxact:name>device</ipxact:name>
          <ipxact:displayName>Device</ipxact:displayName>
          <ipxact:value>A5EB013BB23BE4SCS</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceFamily" type="string">
          <ipxact:name>deviceFamily</ipxact:name>
          <ipxact:displayName>Device family</ipxact:displayName>
          <ipxact:value>Agilex 5</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="deviceSpeedGrade" type="string">
          <ipxact:name>deviceSpeedGrade</ipxact:name>
          <ipxact:displayName>Device Speed Grade</ipxact:displayName>
          <ipxact:value>4</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="generationId" type="int">
          <ipxact:name>generationId</ipxact:name>
          <ipxact:displayName>Generation Id</ipxact:displayName>
          <ipxact:value>0</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="bonusData" type="string">
          <ipxact:name>bonusData</ipxact:name>
          <ipxact:displayName>bonusData</ipxact:displayName>
          <ipxact:value>bonusData 
{
   element EMIF_Qsys_emif_ddr4a_0
   {
      datum _sortIndex
      {
         value = "0";
         type = "int";
      }
   }
}
</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="hideFromIPCatalog" type="bit">
          <ipxact:name>hideFromIPCatalog</ipxact:name>
          <ipxact:displayName>Hide from IP Catalog</ipxact:displayName>
          <ipxact:value>false</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="lockedInterfaceDefinition" type="string">
          <ipxact:name>lockedInterfaceDefinition</ipxact:name>
          <ipxact:displayName>lockedInterfaceDefinition</ipxact:displayName>
          <ipxact:value>&lt;boundaryDefinition&gt;
    &lt;interfaces&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4_clock_in&lt;/name&gt;
            &lt;type&gt;clock&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_clock_in&lt;/name&gt;
                    &lt;role&gt;clk&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;clockRate&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;externallyDriven&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ptfSchematicName&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;core_init_n&lt;/name&gt;
            &lt;type&gt;reset&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;core_init_n&lt;/name&gt;
                    &lt;role&gt;reset_n&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;synchronousEdges&lt;/key&gt;
                        &lt;value&gt;NONE&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4_ctrl_ready&lt;/name&gt;
            &lt;type&gt;reset&lt;/type&gt;
            &lt;isStart&gt;true&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_reset_n&lt;/name&gt;
                    &lt;role&gt;reset_n&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedDirectReset&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedResetSinks&lt;/key&gt;
                        &lt;value&gt;none&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;synchronousEdges&lt;/key&gt;
                        &lt;value&gt;NONE&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4&lt;/name&gt;
            &lt;type&gt;axi4&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awaddr&lt;/name&gt;
                    &lt;role&gt;awaddr&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;30&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awburst&lt;/name&gt;
                    &lt;role&gt;awburst&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awid&lt;/name&gt;
                    &lt;role&gt;awid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;7&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awlen&lt;/name&gt;
                    &lt;role&gt;awlen&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;8&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awlock&lt;/name&gt;
                    &lt;role&gt;awlock&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awqos&lt;/name&gt;
                    &lt;role&gt;awqos&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awsize&lt;/name&gt;
                    &lt;role&gt;awsize&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awvalid&lt;/name&gt;
                    &lt;role&gt;awvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awuser&lt;/name&gt;
                    &lt;role&gt;awuser&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;14&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awprot&lt;/name&gt;
                    &lt;role&gt;awprot&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_awready&lt;/name&gt;
                    &lt;role&gt;awready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_araddr&lt;/name&gt;
                    &lt;role&gt;araddr&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;30&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arburst&lt;/name&gt;
                    &lt;role&gt;arburst&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arid&lt;/name&gt;
                    &lt;role&gt;arid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;7&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arlen&lt;/name&gt;
                    &lt;role&gt;arlen&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;8&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arlock&lt;/name&gt;
                    &lt;role&gt;arlock&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arqos&lt;/name&gt;
                    &lt;role&gt;arqos&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arsize&lt;/name&gt;
                    &lt;role&gt;arsize&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arvalid&lt;/name&gt;
                    &lt;role&gt;arvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_aruser&lt;/name&gt;
                    &lt;role&gt;aruser&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;14&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arprot&lt;/name&gt;
                    &lt;role&gt;arprot&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_arready&lt;/name&gt;
                    &lt;role&gt;arready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_wdata&lt;/name&gt;
                    &lt;role&gt;wdata&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;256&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_wstrb&lt;/name&gt;
                    &lt;role&gt;wstrb&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;32&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_wlast&lt;/name&gt;
                    &lt;role&gt;wlast&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_wvalid&lt;/name&gt;
                    &lt;role&gt;wvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_wready&lt;/name&gt;
                    &lt;role&gt;wready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_bready&lt;/name&gt;
                    &lt;role&gt;bready&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_bid&lt;/name&gt;
                    &lt;role&gt;bid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;7&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_bresp&lt;/name&gt;
                    &lt;role&gt;bresp&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_bvalid&lt;/name&gt;
                    &lt;role&gt;bvalid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rready&lt;/name&gt;
                    &lt;role&gt;rready&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rdata&lt;/name&gt;
                    &lt;role&gt;rdata&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;256&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rid&lt;/name&gt;
                    &lt;role&gt;rid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;7&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rlast&lt;/name&gt;
                    &lt;role&gt;rlast&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rresp&lt;/name&gt;
                    &lt;role&gt;rresp&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4_rvalid&lt;/name&gt;
                    &lt;role&gt;rvalid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;mem_capacity_gbits&lt;/key&gt;
                        &lt;value&gt;8.0&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/assignmentValueMap&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                        &lt;value&gt;s0_axi4_clock_in&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                        &lt;value&gt;s0_axi4_ctrl_ready&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;trustzoneAware&lt;/key&gt;
                        &lt;value&gt;true&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;wakeupSignals&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;uniqueIdSupport&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;poison&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;traceSignals&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;isTranslator&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingReads&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingWrites&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingTransactions&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dataCheck&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;addressCheck&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;securityAttribute&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;userData&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;readAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;64&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;writeAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;64&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;combinedAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;64&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;readDataReorderingDepth&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;bridgesToMaster&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureGuid&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhGroupId&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterId&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterName&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterVersion&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterData&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterDataLength&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureMajorVersion&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureMinorVersion&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureId&lt;/key&gt;
                        &lt;value&gt;35&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureType&lt;/key&gt;
                        &lt;value&gt;3&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4lite_clock&lt;/name&gt;
            &lt;type&gt;clock&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_clock&lt;/name&gt;
                    &lt;role&gt;clk&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;clockRate&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;externallyDriven&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ptfSchematicName&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4lite_reset_n&lt;/name&gt;
            &lt;type&gt;reset&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_reset_n&lt;/name&gt;
                    &lt;role&gt;reset_n&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                        &lt;value&gt;s0_axi4lite_clock&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;synchronousEdges&lt;/key&gt;
                        &lt;value&gt;DEASSERT&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;s0_axi4lite&lt;/name&gt;
            &lt;type&gt;axi4lite&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_awaddr&lt;/name&gt;
                    &lt;role&gt;awaddr&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;27&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_awprot&lt;/name&gt;
                    &lt;role&gt;awprot&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_awvalid&lt;/name&gt;
                    &lt;role&gt;awvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_awready&lt;/name&gt;
                    &lt;role&gt;awready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_araddr&lt;/name&gt;
                    &lt;role&gt;araddr&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;27&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_arprot&lt;/name&gt;
                    &lt;role&gt;arprot&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;3&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_arvalid&lt;/name&gt;
                    &lt;role&gt;arvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_arready&lt;/name&gt;
                    &lt;role&gt;arready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_wdata&lt;/name&gt;
                    &lt;role&gt;wdata&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;32&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_wstrb&lt;/name&gt;
                    &lt;role&gt;wstrb&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_wvalid&lt;/name&gt;
                    &lt;role&gt;wvalid&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_wready&lt;/name&gt;
                    &lt;role&gt;wready&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_bready&lt;/name&gt;
                    &lt;role&gt;bready&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_bresp&lt;/name&gt;
                    &lt;role&gt;bresp&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_bvalid&lt;/name&gt;
                    &lt;role&gt;bvalid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_rready&lt;/name&gt;
                    &lt;role&gt;rready&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_rdata&lt;/name&gt;
                    &lt;role&gt;rdata&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;32&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_rresp&lt;/name&gt;
                    &lt;role&gt;rresp&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;2&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;s0_axi4lite_rvalid&lt;/name&gt;
                    &lt;role&gt;rvalid&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                        &lt;value&gt;s0_axi4lite_clock&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                        &lt;value&gt;s0_axi4lite_reset_n&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;trustzoneAware&lt;/key&gt;
                        &lt;value&gt;true&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;wakeupSignals&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;uniqueIdSupport&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;poison&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;traceSignals&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;isTranslator&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingReads&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingWrites&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;maximumOutstandingTransactions&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dataCheck&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;addressCheck&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;securityAttribute&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;userData&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;readAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;writeAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;combinedAcceptanceCapability&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;readDataReorderingDepth&lt;/key&gt;
                        &lt;value&gt;1&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;bridgesToMaster&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureGuid&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhGroupId&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterId&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterName&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterVersion&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterData&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhParameterDataLength&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureMajorVersion&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureMinorVersion&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureId&lt;/key&gt;
                        &lt;value&gt;35&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;dfhFeatureType&lt;/key&gt;
                        &lt;value&gt;3&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;mem_0&lt;/name&gt;
            &lt;type&gt;conduit&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_cs&lt;/name&gt;
                    &lt;role&gt;mem_cs&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_ca&lt;/name&gt;
                    &lt;role&gt;mem_ca&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;6&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_cke&lt;/name&gt;
                    &lt;role&gt;mem_cke&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_dq&lt;/name&gt;
                    &lt;role&gt;mem_dq&lt;/role&gt;
                    &lt;direction&gt;Bidir&lt;/direction&gt;
                    &lt;width&gt;32&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_dqs_t&lt;/name&gt;
                    &lt;role&gt;mem_dqs_t&lt;/role&gt;
                    &lt;direction&gt;Bidir&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_dqs_c&lt;/name&gt;
                    &lt;role&gt;mem_dqs_c&lt;/role&gt;
                    &lt;direction&gt;Bidir&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_dmi&lt;/name&gt;
                    &lt;role&gt;mem_dmi&lt;/role&gt;
                    &lt;direction&gt;Bidir&lt;/direction&gt;
                    &lt;width&gt;4&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;prSafe&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;mem_ck_0&lt;/name&gt;
            &lt;type&gt;conduit&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_ck_t&lt;/name&gt;
                    &lt;role&gt;mem_ck_t&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_ck_c&lt;/name&gt;
                    &lt;role&gt;mem_ck_c&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC_VECTOR&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;prSafe&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;mem_reset_n&lt;/name&gt;
            &lt;type&gt;conduit&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;mem_0_reset_n&lt;/name&gt;
                    &lt;role&gt;mem_reset_n&lt;/role&gt;
                    &lt;direction&gt;Output&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;prSafe&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;oct_0&lt;/name&gt;
            &lt;type&gt;conduit&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;oct_rzqin_0&lt;/name&gt;
                    &lt;role&gt;oct_rzqin&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedClock&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;associatedReset&lt;/key&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;prSafe&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
        &lt;interface&gt;
            &lt;name&gt;ref_clk&lt;/name&gt;
            &lt;type&gt;clock&lt;/type&gt;
            &lt;isStart&gt;false&lt;/isStart&gt;
            &lt;ports&gt;
                &lt;port&gt;
                    &lt;name&gt;ref_clk&lt;/name&gt;
                    &lt;role&gt;clk&lt;/role&gt;
                    &lt;direction&gt;Input&lt;/direction&gt;
                    &lt;width&gt;1&lt;/width&gt;
                    &lt;lowerBound&gt;0&lt;/lowerBound&gt;
                    &lt;vhdlType&gt;STD_LOGIC&lt;/vhdlType&gt;
                    &lt;terminationValue&gt;0&lt;/terminationValue&gt;
                &lt;/port&gt;
            &lt;/ports&gt;
            &lt;assignments&gt;
                &lt;assignmentValueMap/&gt;
            &lt;/assignments&gt;
            &lt;parameters&gt;
                &lt;parameterValueMap&gt;
                    &lt;entry&gt;
                        &lt;key&gt;clockRate&lt;/key&gt;
                        &lt;value&gt;0&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;externallyDriven&lt;/key&gt;
                        &lt;value&gt;false&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ptfSchematicName&lt;/key&gt;
                    &lt;/entry&gt;
                &lt;/parameterValueMap&gt;
            &lt;/parameters&gt;
        &lt;/interface&gt;
    &lt;/interfaces&gt;
&lt;/boundaryDefinition&gt;</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="systemInfos" type="string">
          <ipxact:name>systemInfos</ipxact:name>
          <ipxact:displayName>systemInfos</ipxact:displayName>
          <ipxact:value>&lt;systemInfosDefinition&gt;
    &lt;connPtSystemInfos&gt;
        &lt;entry&gt;
            &lt;key&gt;s0_axi4&lt;/key&gt;
            &lt;value&gt;
                &lt;connectionPointName&gt;s0_axi4&lt;/connectionPointName&gt;
                &lt;suppliedSystemInfos/&gt;
                &lt;consumedSystemInfos&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_MAP&lt;/key&gt;
                        &lt;value&gt;&amp;lt;address-map&amp;gt;&amp;lt;slave name='s0_axi4' start='0x0' end='0x40000000' datawidth='256' /&amp;gt;&amp;lt;/address-map&amp;gt;&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;ADDRESS_WIDTH&lt;/key&gt;
                        &lt;value&gt;30&lt;/value&gt;
                    &lt;/entry&gt;
                    &lt;entry&gt;
                        &lt;key&gt;MAX_SLAVE_DATA_WIDTH&lt;/key&gt;
                        &lt;value&gt;256&lt;/value&gt;
                    &lt;/entry&gt;
                &lt;/consumedSystemInfos&gt;
            &lt;/value&gt;
        &lt;/entry&gt;
    &lt;/connPtSystemInfos&gt;
&lt;/systemInfosDefinition&gt;</ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="dflBitArray" type="string">
          <ipxact:name>dflBitArray</ipxact:name>
          <ipxact:displayName>dflBitArray</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
        <ipxact:parameter parameterId="cpuInfo" type="string">
          <ipxact:name>cpuInfo</ipxact:name>
          <ipxact:displayName>cpuInfo</ipxact:displayName>
          <ipxact:value></ipxact:value>
        </ipxact:parameter>
      </ipxact:parameters>
    </altera:altera_system_parameters>
    <altera:altera_interface_boundary>
      <altera:interface_mapping altera:name="core_init_n" altera:internal="EMIF_Qsys_emif_ddr4a_0.core_init_n" altera:type="reset" altera:dir="end">
        <altera:port_mapping altera:name="core_init_n" altera:internal="core_init_n"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="mem_0" altera:internal="EMIF_Qsys_emif_ddr4a_0.mem_0" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="mem_0_ca" altera:internal="mem_0_ca"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_cke" altera:internal="mem_0_cke"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_cs" altera:internal="mem_0_cs"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_dmi" altera:internal="mem_0_dmi"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_dq" altera:internal="mem_0_dq"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_dqs_c" altera:internal="mem_0_dqs_c"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_dqs_t" altera:internal="mem_0_dqs_t"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="mem_1" altera:internal="EMIF_Qsys_emif_ddr4a_0.mem_1"></altera:interface_mapping>
      <altera:interface_mapping altera:name="mem_ck_0" altera:internal="EMIF_Qsys_emif_ddr4a_0.mem_ck_0" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="mem_0_ck_c" altera:internal="mem_0_ck_c"></altera:port_mapping>
        <altera:port_mapping altera:name="mem_0_ck_t" altera:internal="mem_0_ck_t"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="mem_ck_1" altera:internal="EMIF_Qsys_emif_ddr4a_0.mem_ck_1"></altera:interface_mapping>
      <altera:interface_mapping altera:name="mem_reset_n" altera:internal="EMIF_Qsys_emif_ddr4a_0.mem_reset_n" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="mem_0_reset_n" altera:internal="mem_0_reset_n"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="oct_0" altera:internal="EMIF_Qsys_emif_ddr4a_0.oct_0" altera:type="conduit" altera:dir="end">
        <altera:port_mapping altera:name="oct_rzqin_0" altera:internal="oct_rzqin_0"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="oct_1" altera:internal="EMIF_Qsys_emif_ddr4a_0.oct_1"></altera:interface_mapping>
      <altera:interface_mapping altera:name="ref_clk" altera:internal="EMIF_Qsys_emif_ddr4a_0.ref_clk" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="ref_clk" altera:internal="ref_clk"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4" altera:type="axi4" altera:dir="end">
        <altera:port_mapping altera:name="s0_axi4_araddr" altera:internal="s0_axi4_araddr"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arburst" altera:internal="s0_axi4_arburst"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arid" altera:internal="s0_axi4_arid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arlen" altera:internal="s0_axi4_arlen"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arlock" altera:internal="s0_axi4_arlock"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arprot" altera:internal="s0_axi4_arprot"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arqos" altera:internal="s0_axi4_arqos"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arready" altera:internal="s0_axi4_arready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arsize" altera:internal="s0_axi4_arsize"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_aruser" altera:internal="s0_axi4_aruser"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_arvalid" altera:internal="s0_axi4_arvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awaddr" altera:internal="s0_axi4_awaddr"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awburst" altera:internal="s0_axi4_awburst"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awid" altera:internal="s0_axi4_awid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awlen" altera:internal="s0_axi4_awlen"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awlock" altera:internal="s0_axi4_awlock"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awprot" altera:internal="s0_axi4_awprot"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awqos" altera:internal="s0_axi4_awqos"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awready" altera:internal="s0_axi4_awready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awsize" altera:internal="s0_axi4_awsize"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awuser" altera:internal="s0_axi4_awuser"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_awvalid" altera:internal="s0_axi4_awvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_bid" altera:internal="s0_axi4_bid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_bready" altera:internal="s0_axi4_bready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_bresp" altera:internal="s0_axi4_bresp"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_bvalid" altera:internal="s0_axi4_bvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rdata" altera:internal="s0_axi4_rdata"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rid" altera:internal="s0_axi4_rid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rlast" altera:internal="s0_axi4_rlast"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rready" altera:internal="s0_axi4_rready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rresp" altera:internal="s0_axi4_rresp"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_rvalid" altera:internal="s0_axi4_rvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_wdata" altera:internal="s0_axi4_wdata"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_wlast" altera:internal="s0_axi4_wlast"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_wready" altera:internal="s0_axi4_wready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_wstrb" altera:internal="s0_axi4_wstrb"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4_wvalid" altera:internal="s0_axi4_wvalid"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4_clock_in" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4_clock_in" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="s0_axi4_clock_in" altera:internal="s0_axi4_clock_in"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4_ctrl_ready" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4_ctrl_ready" altera:type="reset" altera:dir="start">
        <altera:port_mapping altera:name="s0_axi4_reset_n" altera:internal="s0_axi4_reset_n"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4lite" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4lite" altera:type="axi4lite" altera:dir="end">
        <altera:port_mapping altera:name="s0_axi4lite_araddr" altera:internal="s0_axi4lite_araddr"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_arprot" altera:internal="s0_axi4lite_arprot"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_arready" altera:internal="s0_axi4lite_arready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_arvalid" altera:internal="s0_axi4lite_arvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_awaddr" altera:internal="s0_axi4lite_awaddr"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_awprot" altera:internal="s0_axi4lite_awprot"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_awready" altera:internal="s0_axi4lite_awready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_awvalid" altera:internal="s0_axi4lite_awvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_bready" altera:internal="s0_axi4lite_bready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_bresp" altera:internal="s0_axi4lite_bresp"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_bvalid" altera:internal="s0_axi4lite_bvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_rdata" altera:internal="s0_axi4lite_rdata"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_rready" altera:internal="s0_axi4lite_rready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_rresp" altera:internal="s0_axi4lite_rresp"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_rvalid" altera:internal="s0_axi4lite_rvalid"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_wdata" altera:internal="s0_axi4lite_wdata"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_wready" altera:internal="s0_axi4lite_wready"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_wstrb" altera:internal="s0_axi4lite_wstrb"></altera:port_mapping>
        <altera:port_mapping altera:name="s0_axi4lite_wvalid" altera:internal="s0_axi4lite_wvalid"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4lite_clock" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4lite_clock" altera:type="clock" altera:dir="end">
        <altera:port_mapping altera:name="s0_axi4lite_clock" altera:internal="s0_axi4lite_clock"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s0_axi4lite_reset_n" altera:internal="EMIF_Qsys_emif_ddr4a_0.s0_axi4lite_reset_n" altera:type="reset" altera:dir="end">
        <altera:port_mapping altera:name="s0_axi4lite_reset_n" altera:internal="s0_axi4lite_reset_n"></altera:port_mapping>
      </altera:interface_mapping>
      <altera:interface_mapping altera:name="s1_axi4" altera:internal="EMIF_Qsys_emif_ddr4a_0.s1_axi4"></altera:interface_mapping>
    </altera:altera_interface_boundary>
    <altera:altera_has_warnings>false</altera:altera_has_warnings>
    <altera:altera_has_errors>false</altera:altera_has_errors>
  </ipxact:vendorExtensions>
</ipxact:component>